DICOM PS3.3 2016b - Information Object Definitions

C.8.8.15.3 Channel Length
Prev | C.8.8.15 RT Brachy Application Setups Module | Next

##### C.8.8.15.3 Channel Length

If specified, Channel Length (300A,0284) shall be the sum of the Source Applicator Length (300A,0296) and Transfer Tube Length (300A,02A4).

Prev | Up | Next
C.8.8.15.2 Referenced ROI Number | Home | C.8.8.15.4 Oscillating Source Movement

DICOM PS3.3 2016b - Information Object Definitions