DICOM PS3.3 2016c - Information Object Definitions

C.13 Print Management Specific Modules
Prev | C Information Module Definitions (Normative) | Next

## C.13 Print Management Specific Modules

The following Sections specify Modules used for Print Management.

### C.13.1 Basic Film Session Presentation Module

Table C.13-1. Basic Film Session Presentation Module Attributes

Attribute name | Tag | Attribute Description
--- | --- | ---
Number of Copies | (2000,0010) | Number of copies to be printed for each film of the film session.
Print Priority | (2000,0020) | Specifies the priority of the print job. Enumerated Values: HIGH MED LOW
Medium Type | (2000,0030) | Type of medium on which the print job will be printed. Defined Terms: PAPER CLEAR FILM BLUE FILM MAMMO CLEAR FILM MAMMO BLUE FILM
Film Destination | (2000,0040) | Film destination. Defined Terms: MAGAZINE the exposed film is stored in film magazine PROCESSOR the exposed film is developed in film processor BIN_i the exposed film is deposited in a sorter bin where "I" represents the bin number. Film sorter BINs shall be numbered sequentially starting from 1 and no maximum is placed on the number of BINs. The encoding of the BIN number shall not contain leading zeros.
Film Session Label | (2000,0050) | Human readable label that identifies the film session
Memory Allocation | (2000,0060) | Amount of memory allocated for the film session. Value is expressed in KB
Owner ID | (2100,0160) | Identification of the owner of the film session

Prev | Up | Next
C.12.3 Frame Extraction Module | Home | C.13.2 Basic Film Session Relationship Module

DICOM PS3.3 2016c - Information Object Definitions