DICOM PS3.3 2016c - Information Object Definitions

A.51.4 Segmentation IOD Content Constraints
Prev | A.51 Segmentation IOD | Next

### A.51.4 Segmentation IOD Content Constraints

The VOI LUT Module shall not be present.

The Modality LUT Module shall not be present.

The Overlay Plane Module shall not be present.

Pixel Padding Value (0028,0120) shall not be present.

Prev | Up | Next
A.51.3 Segmentation IOD Module Table | Home | A.51.5 Segmentation Functional Groups

DICOM PS3.3 2016c - Information Object Definitions