DICOM PS3.7 2016c - Message Exchange

C.4.3 Attribute Value Out of Range
Prev | C.4 Warning Status Class | Next

### C.4.3 Attribute Value Out of Range

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0116H.
Modification List/Attribute List | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid Attribute Values conveyed in the Modification List of the N-SET-RQ or the Attribute List of the N-CREATE-RQ.

Prev | Up | Next
C.4.2 Attribute List Error | Home | C.5 Failure Status Class

DICOM PS3.7 2016c - Message Exchange