DICOM PS3.3 2016c - Information Object Definitions

A.41 Ophthalmic Photography 8 Bit Image IOD
Prev | A Composite Information Object Definitions (Normative) | Next

## A.41 Ophthalmic Photography 8 Bit Image IOD

This Section defines an Information Object to be used with several types of ophthalmic photographic imaging devices including fundus cameras, slit lamp cameras, scanning laser devices, stereoscopic cameras, video equipment and digital photographic equipment, with 8 bit resolution per pixel in each image plane.

### A.41.1 Ophthalmic Photography 8 Bit Image IOD Description

The Ophthalmic Photography 8 Bit Image IOD specifies a single-frame or a multi-frame image acquired on a digital photographic DICOM modality. This IOD can be used to encode single ophthalmic images and cine sequences.

Prev | Up | Next
A.40.3 Spatial Fiducials IOD Module Table | Home | A.41.2 Ophthalmic Photography 8 Bit Image IOD Entity-Relationship Model

DICOM PS3.3 2016c - Information Object Definitions