DICOM PS3.3 2016c - Information Object Definitions

F.5.23 Presentation State Directory Record Definition
Prev | F.5 Definition of Specific Directory Records | Next

### F.5.23 Presentation State Directory Record Definition

The Directory Record is based on the specification of Section F.3. It is identified by a Directory Record Type of Value "PRESENTATION". Table F.5-23 lists the set of keys with their associated Types for such a Directory Record Type. The description of these keys may be found in the Modules related to Softcopy Presentation State Storage and Structured Display IODs. This Directory Record shall be used to reference a Softcopy Presentation State Storage SOP Instance or a Structured Display SOP Instance. This Type of Directory Record may reference a Lower-Level Directory Entity that includes one or more Directory Records as defined in Table F.4-1.

Table F.5-23. Presentation Keys

Key | Tag | Type | Attribute Description
--- | --- | --- | ---
Specific Character Set | (0008,0005) | 1C | Required if an extended or replacement character set is used in one of the keys.
Presentation Creation Date | (0070,0082) | 1 | Date on which this presentation was created. ### Note This date may be different from the date that the DICOM SOP Instance was created, since the presentation information contained may have been recorded earlier.
Presentation Creation Time | (0070,0083) | 1 | Time at which this presentation was created. ### Note This time may be different from the time that the DICOM SOP Instance was created, since the presentation information contained may have been recorded earlier.
Include Table 10-12 “Content Identification Macro Attributes” |
Referenced Series Sequence | (0008,1115) | 1C | Sequence of Items where each Item includes the Attributes of one Series to which the Presentation applies. One or more Items shall be included in this Sequence. Required if the IOD of the Presentation SOP Instance referenced by this directory record includes the Presentation State Relationship Module.
>Series Instance UID | (0020,000E) | 1 | Unique identifier of a Series that is part of this Study.
>Referenced Image Sequence | (0008,1140) | 1 | Sequence of Items where each Item provides reference to an Image SOP Instance. One or more Items shall be included in this Sequence.
>>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
Blending Sequence | (0070,0402) | 1C | Sequence of Items where each Item includes the Attributes of a Study to which the Presentation applies. Only two Items shall be included in this Sequence. Required if the SOP Instance referenced by this directory record includes Blending Sequence (0070,0402).
>Study Instance UID | (0020,000D) | 1 | Unique identifier for a Study that contains the images to which the Presentation applies.
>Referenced Series Sequence | (0008,1115) | 1 | Sequence of Items where each Item includes the Attributes of one Series to which the Presentation applies. Only a single Item shall be included in this Sequence.
>>Series Instance UID | (0020,000E) | 1 | Unique identifier of the Series
>>Referenced Image Sequence | (0008,1140) | 1 | Sequence of Items where each Item provides reference to an Image SOP Instance to which the Presentation applies. One or more Items shall be included in this Sequence.
>>>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
Any other Attribute of the Presentation State IE Modules | 3 |

### Note

Because Referenced SOP Instance UID in File (0004,1511) may be used as a "pseudo" Directory Record Key (see Table F.3-3), it is not duplicated in this list of keys.

Prev | Up | Next
F.5.22 RT Treatment Record Directory Record Definition | Home | F.5.24 Waveform Directory Record Definition

DICOM PS3.3 2016c - Information Object Definitions