DICOM PS3.17 2016c - Explanatory Information

XXX.3.8.3 Encoding Details
Prev | XXX.3.8 Blending with Functional Data, e.g. PET/CT or Perfusion Data | Next

#### XXX.3.8.3 Encoding Details

##### XXX.3.8.3.1 Volumetric Presentation State Relationship Module Recommendations

Table XXX.3.8-1. Volumetric Presentation State Relationship Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Volumetric Presentation State Input Sequence | (0070,1201) | Contains two items: one for the CT volume input and one for the PET volume input.
>ITEM 1
>Presentation Input Type | (0070,1202) | Set to "VOLUME".
>Referenced Image Sequence | (0008,1140) | Set reference(s) to the image(s) that make(s) up the CT input volume.
>Referenced Spatial Registration Sequence | (0070,0404) | Set to reference the Spatial Registration instance which registers the CT input to the VPS RCS.
>Window Center | (0028,1050) | Set either Window Center and Window Width or VOI LUT Sequence (0028,3010).
>Window Width | (0028,1051) |
>Crop | (0070,1204) | Set to "NO".
>ITEM 2
>Presentation Input Type | (0070,1202) | Set to "VOLUME".
>Referenced Image Sequence | (0008,1140) | Set reference(s) to the image(s) that make(s) up the PET input volume.
>Referenced Spatial Registration Sequence | (0070,0404) | Set reference to the Spatial Registration instance which registers the PET input to the VPS RCS.
>Window Center | (0028,1050) | Set either Window Center and Window Width or VOI LUT Sequence (0028,3010).
>Window Width | (0028,1051) |
>Crop | (0070,1204) | Set to "NO".

Prev | Up | Next
XXX.3.8.2 Encoding Outline | Home | XXX.3.8.2.3 Volumetric Presentation State Display Module Recommendations

DICOM PS3.17 2016c - Explanatory Information