DICOM PS3.3 2016c - Information Object Definitions

C.30.3 Unified Procedure Step Performed Procedure Information Module
Prev | C.30 Unified Procedure Step Specific Modules | Next

### C.30.3 Unified Procedure Step Performed Procedure Information Module

Table C.30.3-1 specifies the Attributes that describe the performance and results of a Unified Procedure Step (UPS).

Table C.30.3-1. Unified Procedure Step Performed Procedure Information Module Attributes

Attribute Name | Tag | Attribute Description
--- | --- | ---
Unified Procedure Step Performed Procedure Sequence | (0074,1216) | Details of the Procedure Step as performed. Zero or one Item shall be included in this Sequence.
>Actual Human Performers Sequence | (0040,4035) | Human performers that are/were actually involved or responsible for performing the Procedure Step. Zero or more Items shall be included in this Sequence. ### Note Initially this list will be empty. Items may be added to the list at or after the status transition of the Procedure Step State (0074,1000) to "IN PROGRESS"
>>Human Performer Code Sequence | (0040,4009) | Human performer that is involved or responsible for performing the Procedure Step. Only a single Item shall be included in this Sequence.
>>>Include Table 8.8-1 “Code Sequence Macro Attributes” | No Baseline CID is defined.
>>Human Performer's Name | (0040,4037) | Name of the human performer.
>>Human Performer's Organization | (0040,4036) | Organization to which the human performer is accountable for the activities in the Procedure Step.
>Performed Station Name Code Sequence | (0040,4028) | Names within the enterprise of the equipment that performed the Procedure Step. This name may be the same as the AE Title, but does not have to be. Zero or more Items shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | No Baseline CID is defined.
>Performed Station Class Code Sequence | (0040,4029) | Classes of the equipment that created the Procedure Step. Zero or more Items shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | No Baseline CID is defined.
>Performed Station Geographic Location Code Sequence | (0040,4030) | Geographic locations of the equipment that created Procedure Step. Zero or more Items shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | No Baseline CID is defined.
>Performed Procedure Step Start DateTime | (0040,4050) | Date and Time at which the Procedure Step started.
>Performed Procedure Step Description | (0040,0254) | Institution-generated description or classification of the Procedure Step that was performed.
>Comments on the Performed Procedure Step | (0040,0280) | User-defined comments on the Performed Procedure Step.
>Performed Workitem Code Sequence | (0040,4019) | A sequence that conveys the type of procedure performed. Zero or more items shall be present in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | Baseline CID is CID 9231 “Workitem Definition”. ### Note This CID has generic workitems. An implementation may choose to define more specific, detailed workitems.
>Performed Processing Parameters Sequence | (0074,1212) | Parameters used to perform the procedure. Zero or more items shall be present in this Sequence
>>Include Table 10-2 “Content Item Macro Attributes Description” | No Baseline CIDs are defined for Concept Name Code Sequence or Concept Code Sequence.
>>Content Item Modifier Sequence | (0040,0441) | Sequence that specifies modifiers for a Protocol Context Content Item. One or more Items are permitted in this Sequence.
>>>Include Table 10-2 “Content Item Macro Attributes Description” | No Baseline CIDs are defined for Concept Name Code Sequence or Concept Code Sequence.
>Performed Procedure Step End DateTime | (0040,4051) | Date and Time at which the Procedure Step ended.
>Output Information Sequence | (0040,4033) | References to information created as part of the Procedure Step. Referencing unencapsulated HL7 documents is described further in Section C.12.1.1.6. Zero or more Items shall be included in this Sequence.
>>Include Table 10-3b “Referenced Instances and Access Macro Attributes” |

Prev | Up | Next
C.30.2 Unified Procedure Step Scheduled Procedure Information Module | Home | C.30.4 Unified Procedure Step Relationship Module

DICOM PS3.3 2016c - Information Object Definitions