DICOM PS3.11 2016c - Media Storage Application Profiles

L.4.5 Specific Image Requirements For STD-DTL-SEC-ZIP-MAIL
Prev | L.4 Dental Class Profile | Next

### L.4.5 Specific Image Requirements For STD-DTL-SEC-ZIP-MAIL

For Digital Intra-oral X-Ray Image and Digital X-Ray Image Instances interchanged under the STD-DTL-SEC-ZIP-MAIL profile, the Attributes listed in Table L.4-1 used within the image instances shall take the values specified.

Table L.4-1. STD-DTL-ZIP-MAIL - Required Image Attribute Values

Attribute | Tag | Value
--- | --- | ---
Bits Allocated | (0028,0100) | If Bits Stored (0028,0101) is 8, then 8; otherwise 16.
Bits Stored | (0028,0101) | 8, 10, 12 or 16

The Attributes listed in Table L.4-2 shall have their Types specialized.

Table L.4-2. STD-DTL-ZIP-MAIL - Required Image Attribute Types

Attribute | Tag | Type
--- | --- | ---
Institution Name | (0008,0080) | 2
Manufacturer's Model Name | (0008,1090) | 2
Detector ID | (0018,700A) | 2
Detector Manufacturer Name | (0018,702A) | 2
Detector Manufacturer's Model Name | (0018,702B) | 2

### Note

These Type 3 attributes of the General Equipment and DX Detector Module are specialized in order to encourage FSCs to include values for them, recognizing that there are situations in which values may be unknown.

Prev | Up | Next
L.4.3 Directory Information in DICOMDIR | Home | L.4.6 Secure Transport

DICOM PS3.11 2016c - Media Storage Application Profiles