DICOM PS3.17 2016c - Explanatory Information

XXX.5.2 Partially Transparent A Over B Compositing
Prev | XXX.5 Compositing and the Use of Weighting Transfer Functions | Next

### XXX.5.2 Partially Transparent A Over B Compositing

In this example, the Compositor Component performs a Porter-Duff "Partially Transparent A over B" compositing.

Figure XXX.5-2. Weighting LUTs for Partially Transparent A Over B Compositing

Prev | Up | Next
XXX.5 Compositing and the Use of Weighting Transfer Functions | Home | XXX.5.3 Pass-through Compositing

DICOM PS3.17 2016c - Explanatory Information