DICOM PS3.17 2016c - Explanatory Information

PPP.3.2 An Example of A Tablet Display
Prev | PPP.3 Examples of Display System SOP Class | Next

### PPP.3.2 An Example of A Tablet Display

A Tablet Display System is shown in Figure PPP.3.2-1.

Figure PPP.3.2-1. A Tablet Display System

The following is an example of an N-GET Request/Response pair for the Display System SOP Class.

This example is encoded with Undefined Sequence Length and Undefined Item Length, so it contains Sequence Delimitation Items and Item Delimitation Items.

N-GET:

ANP

  Attribute Not Present.

VNP

  Attribute Present but Value Not Present.

-

  Not specified.

Table PPP.3.2-1. N-GET Request/Response Example

Attribute Name | Tag | N-GET Request (SCU) | N-GET Response (SCP)
--- | --- | --- | ---
SOP Common and Workstation Modules
Specific Character Set | (0008,0005) | ANP | \ISO 2022 IR 87
Manufacturer | (0008,0070) | VNP | Tablet Corp.
Institution Name | (0008,0080) | VNP | JIRA Hospital
Institution Address | (0008,0081) | VNP | Bunkyo-ku, Tokyo, Japan
Device Serial Number | (0018,1000) | VNP | AA1B22CCCC3D
Station Name | (0008,1010) | VNP | TABLET1
Institutional Department Name | (0008,1040) | VNP | Radiology Dept.
Manufacturer's Model Name | (0008,1090) | VNP | MC706J/A
Equipment Administrator Sequence | (0028,7000) | VNP |
>Item #1 of Equipment Administrator Sequence | (FFFE,E000) | - |
>Person Name | (0040,A123) | - | Yamada^Tarou=山田^太郎=やまだ^たろう
>Person Identification Code Sequence | (0040,1101) | - |
>>Item #1 of Person Identification Code Sequence | (FFFE,E000) | - |
>>Code Value | (0008,0110) | - | 111111
>>Coding Scheme Designator | (0008,0102) | - | LOCAL
>>Code Meaning | (0008,0104) | - | Yamada^Tarou
>>Item Delimiter of Item #1 of Person Identification Code Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Person Identification Code Sequence | (FFFE,E0DD) | - |
>Person's Address | (0040,1102) | - |
>Person's Telephone Number | (0040,1103) | - | EXT. 1234
>Institution Name | (0008,0080) | - | IT Support Div.
>Item Delimiter of Item #1 of Equipment Administrator Sequence | (FFFE,E00D) | - |
>Sequence Delimiter of Equipment Administrator Sequence | (FFFE,E0DD) | - |
Display System Module
Number of Display Subsystems | (0028,7001) | VNP | 1
Display Subsystem Sequence | (0028,7023) | VNP |
Item #1 of Display Subsystem Sequence | (FFFE,E000) | - |
>Display Subsystem ID | (0028,7003) | - | 1
>Display Subsystem Name | (0028,7004) | - | DS1
>Display Subsystem Description | (0028,7005) | - | Embedded LCD
>Display Device Type Code Sequence | (0028,7022) | - |
>>Item #1 of Display Device Type Code Sequence | (FFFE,E000) | - |
>>Code Value | (0008,0100) | - | 109992
>>Coding Scheme Designator | (0008,0102) | - | DCM
>>Code Meaning | (0008,0104) | - | Liquid Crystal Display
>>Item Delimiter of Item #1 of Display Device Type Code Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Device Type Code Sequence | (FFFE,E0DD) | - |
>Manufacturer | (0008,0070) | - | Tablet Corp.
>Device Serial Number | (0018,1000) | - | AA1B22CCCC3D
>Manufacturer's Model Name | (0008,1090) | - | MC706J/A
>System Status | (0028,7006) | - | NORMAL
>System Status Comment | (0028,7007) | - |
>Display Subsystem Configuration Sequence | (0028,700A) | - |
>>Item #1 of Display Subsystem Configuration Sequence | (FFFE,E000) | - |
>>Configuration ID | (0028,700B) | - | 1
>>Configuration Name | (0028,700C) | - | DS1Config1
>> Configuration Description | (0028,700D) | - | Configuration1 of Display Subsystem ID1
>>Referenced Target Luminance Characteristics ID | (0028,700E) | - | 1
>>Item Delimiter of Item #1 of Display Subsystem Configuration Sequence | (FFFE,E00D) | - |
>>Sequence Delimiter of Display Subsystem Configuration Sequence | (FFFE,E0DD) | - |
>Current Configuration ID | (0028,7002) | - | 1
>Measurement Equipment Sequence | (0028,7012) | - |
>Sequence Delimiter of Measurement Equipment Sequence | (FFFE,E0DD) | - |
>Item Delimiter of Item #1 of Display System Sequence | (FFFE,E00D) | - |
>Sequence Delimiter of Display Subsystem Sequence | (FFFE,E0DD) | - |
Target Luminance Characteristics Module
Target Luminance Characteristics Sequence | (0028,7008) | VNP |
>Item #1 of Target Luminance Characteristics Sequence | (FFFE,E000) | - |
>Luminance Characteristics ID | (0028,7009) | - | 1
>Display Function Type | (0028,7019) | - | GAMMA
>Target Minimum Luminance | (0028,701D) | - | 0.75
>Target Maximum Luminance | (0028,701E) | - | 300
>Gamma Value | (0028,701A) | - | 2.2
>Item Delimiter of Item #1 of Target Luminance Characteristics Sequence | (FFFE,E00D) | - |
>Sequence Delimiter of Target Luminance Characteristics Sequence | (FFFE,E0DD) | - |
QA Result Module
QA Results Sequence | (0028,700F) | VNP |
>Item #1 of QA Results Sequence | (FFFE,E000) | - |
>Display Subsystem ID | (0028,7003) | - | 1
>Display Subsystem QA Results Sequence | (0028,7010) | - | There are no items in this sequence in this example.

Prev | Up | Next
PPP.3 Examples of Display System SOP Class | Home | QQQ Parametric Maps (Informative)

DICOM PS3.17 2016c - Explanatory Information