DICOM PS3.16 2016c - Content Mapping Resource

TID 8121 Animal Housing
Prev | Acquisition Context SR IOD Templates | Next

### TID 8121 Animal Housing

This template encodes a description of housing of animals, e.g., in home cages, holders for imaging, etc., over an interval during which environmental and handling conditions are relatively homogenous.

### Note

1. Only "static" parameters of the design and setup are recorded, and "nominal" values for environmental conditions such as humidity and temperature, but not "dynamic" parameters that might vary during one housing interval, and potentially be monitored, such as oxygen or ammonia levels, temperature, humidity, urine or fecal corticosterone levels, etc.

2. Values for product names and codes are expected to be accurate at the time the information is recorded, recognizing that products may evolve over time.

Type:

  Extensible

Order:

  Non-Significant

Table TID 8121. Animal Housing

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (127120, DCM, "Animal housing") | 1 | M |  |
2 | > | CONTAINS | CODE | EV (127121, DCM, "Animal room type") | 1 | U |  | DCID 603 “Animal Room Types”
2b | > | CONTAINS | TEXT | EV (127122, DCM, "Animal room identifier") | 1 | U |  |
3 | > | CONTAINS | TEXT | EV (127125, DCM, "Housing manufacturer") | 1 | U |  |
4 | > | CONTAINS | TEXT | EV (127126, DCM, "Housing rack product name") | 1 | U |  |
5 | > | CONTAINS | TEXT | EV (127127, DCM, "Housing rack product code") | 1 | U |  |
6 | > | CONTAINS | TEXT | EV (127128, DCM, "Housing unit product name") | 1 | U |  |
7 | > | CONTAINS | TEXT | EV (127129, DCM, "Housing unit product code") | 1 | U |  |
8 | > | CONTAINS | TEXT | EV (127130, DCM, "Housing unit lid product name") | 1 | U |  |
9 | > | CONTAINS | TEXT | EV (127131, DCM, "Housing unit lid product code") | 1 | U |  |
10 | > | CONTAINS | NUM | EV (127140, DCM, "Number of racks per room") | 1 | U |  | UNITS = EV ({racks}, UCUM, "racks")
11 | > | CONTAINS | NUM | EV (127141, DCM, "Number of housing units per rack") | 1 | U |  | UNITS = EV ({housing units}, UCUM, "housing units") or EV ({cages}, UCUM, "cages")
12 | > | CONTAINS | TEXT | EV (127142, DCM, "Housing unit location in rack") | 1 | U |  |
13 | > | CONTAINS | NUM | EV (127143, DCM, "Number of animals within same housing unit") | 1 | U |  | UNITS = EV ({animals}, UCUM, "animals")
14 | > | CONTAINS | CODE | EV (127144, DCM, "Sex of animals within same housing unit") | 1 | U |  | DCID 7457 “Sex - Male Female or Both”
15 | > | CONTAINS | CODE | EV (127145, DCM, "Sex of handler") | 1 | U |  | DCID 7457 “Sex - Male Female or Both”
16 | > | CONTAINS | NUM | EV (127150, DCM, "Total duration in housing") | 1 | U |  | UNITS = EV (d, UCUM, "days")
17 | > | CONTAINS | NUM | EV (127151, DCM, "Housing change interval") | 1 | U |  | UNITS = EV (d, UCUM, "days")
18 | > | CONTAINS | NUM | EV (127152, DCM, "Manual handling interval") | 1 | U |  | UNITS = EV (h, UCUM, "hours")
19 | > | CONTAINS | TEXT | EV (127153, DCM, "Housing unit movement") | 1 | U |  |
20 | > | CONTAINS | NUM | EV (127160, DCM, "Housing unit width") | 1 | U |  | UNITS = EV (cm, UCUM, "cm")
21 | > | CONTAINS | NUM | EV (127161, DCM, "Housing unit height") | 1 | U |  | UNITS = EV (cm, UCUM, "cm")
22 | > | CONTAINS | NUM | EV (127162, DCM, "Housing unit length") | 1 | U |  | UNITS = EV (cm, UCUM, "cm")
23 | > | CONTAINS | CODE | EV (127170, DCM, "Housing individually ventilated") | 1 | U |  | DCID 231 “Yes-No Only”
24 | > | CONTAINS | NUM | EV (127172, DCM, "Air changes") | 1 | U |  | UNITS = EV (/h, UCUM, "/hour")
25 | > | CONTAINS | NUM | EV (C90380, NCIt, "Environmental temperature") | 1 | U |  | UNITS = EV (Cel, UCUM, "C")
26 | > | CONTAINS | NUM | EV (C90395, NCIt, "Housing humidity") | 1 | U |  | UNITS = EV (%, UCUM, "%")
27 | > | CONTAINS | CODE | EV (127175, DCM, "Housing unit reuse") | 1 | U |  | DCID 604 “Device Reuse”
28 | > | CONTAINS | CODE | EV (C90366, NCIt, "Bedding material") | 1 | U |  | DCID 605 “Animal Bedding Material”
29 | > | CONTAINS | TEXT | EV (C90366, NCIt, "Bedding material") | 1 | U |  |
30 | > | CONTAINS | TEXT | EV (127180, DCM, "Bedding manufacturer") | 1 | U |  |
31 | > | CONTAINS | TEXT | EV (127181, DCM, "Bedding product name") | 1 | U |  |
32 | > | CONTAINS | TEXT | EV (127182, DCM, "Bedding product code") | 1 | U |  |
33 | > | CONTAINS | NUM | EV (127183, DCM, "Bedding volume") | 1 | U |  | UNITS = EV (ml, UCUM, "ml")
34 | > | CONTAINS | NUM | EV (127184, DCM, "Bedding mass") | 1 | U |  | UNITS = EV (g, UCUM, "g")
34b | > | CONTAINS | NUM | EV (127185, DCM, "Bedding depth") | 1 | U |  | UNITS = EV (mm, UCUM, mm")
35 | > | CONTAINS | NUM | EV (C90365, NCIt, "Bedding change") | 1 | U |  | UNITS = EV (d, UCUM, "days")
36 | > | CONTAINS | CODE | EV (127192, DCM, "Enrichment material present") | 1 | U |  | DCID 241 “Present-Absent Only”
36b | > | CONTAINS | TEXT | EV (127191, DCM, "Enrichment manufacturer") | 1 | U |  |
37 | > | CONTAINS | TEXT | EV (127190, DCM, "Enrichment material") | 1 | U |  |
38 | > | CONTAINS | CODE | EV (127193, DCM, "Exerciser device present") | 1 | U |  | DCID 241 “Present-Absent Only”
39 | > | CONTAINS | TEXT | EV (A-17200, SRT, "Exerciser device") | 1 | U |  |
40 | > | CONTAINS | CODE | EV (127195, DCM, "Shelter type") | 1 | U |  | DCID 606 “Animal Shelter Types”
41 | > | CONTAINS | TEXT | EV (127196, DCM, "Shelter manufacturer") | 1 | U |  |
42 | > | CONTAINS | TEXT | EV (127197, DCM, "Shelter product name") | 1 | U |  |
43 | > | CONTAINS | TEXT | EV (127198, DCM, "Shelter product code") | 1 | U |  |
44 | > | CONTAINS | TEXT | EV (121106, DCM,"Comment") | 1 | U |  |

Content Item Descriptions

Row 2 and 2b | The type and identifier of the entire room in which, for example, one or more racks of housing units is located, not the housing unit itself.
Row 3 | The manufacturer is expected to be the same for all housing unit components, rack, bottom and lid.
Row 12 | The position in the rack is encoded as text since it may be an "identifier" or a description. It is not a set of numeric (e.g., row, column) or coded (e.g., top, bottom or middle) values, since there are too many possible arrangements.
Row 13 | The number of animals usually applies to a single housing unit, but may also be used to describe the number of animals imaged simultaneously in a multi-animal imaging carrier or support device ("chamber", "holder", etc.).
Rows 20-22 | These may be internal or external dimensions, and are intended to provide an approximation of the living space and shape available.
Rows 25-26 | Description of measured or monitored or nominal values of temperature and humidity. The means of maintaining these conditions, if relevant, is described elsewhere (e.g., in the case of peri-procedural temperature control, in TID 8140 “Heating Conditions”).
Rows 28-29 | The bedding material may be described as a code or text, or both. The codes do not distinguish between methods of sterilization of the bedding material (e.g., irradiation, autoclaving or other heat treatment), since that is not a relevant factor for image interpretation. The definition of the NCIt concept is "that which comprises the place where a subject sleeps".
Row 35 | The definition of the NCIt concept is "a replacement of the existing materials that make up the sleeping area of a subject", and is used here to specify the interval between bedding changes.
Row 36-37 | The presence or absence of enrichment material is coded, but the type is not, and may be described as text, e.g., "facial tissue", "cotton (nesting material)".
Row 38-39 | The presence or absence of an exercise device is coded, but the type is not, and may be described as text.

Prev | Up | Next
TID 8110 Biosafety Conditions | Home | TID 8122 Animal Feeding

DICOM PS3.16 2016c - Content Mapping Resource