DICOM PS3.3 2016c - Information Object Definitions

A.34.9.4.6 Waveform Sample Interpretation
Prev | A.34.9.4 Respiratory Waveform IOD Content Constraints | Next

##### A.34.9.4.6 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in each Waveform Sequence Item shall be SB or SS.

Prev | Up | Next
A.34.9.4.5 Channel Source | Home | A.34.10 General Audio Waveform IOD

DICOM PS3.3 2016c - Information Object Definitions