DICOM PS3.17 2016c - Explanatory Information

MM.2.3 Time Interval versus Frame Increment Vector
Prev | MM.2 Frame Extraction Issues | Next

### MM.2.3 Time Interval versus Frame Increment Vector

The Frame Time (0018,1063) may need to be modified if frames in the new image are not a simple contiguous sequence from the original, and if they are irregular, then the Frame Time Vector (0018,1065) will need to be used in its place, with a corresponding change to the Frame Increment Pointer (0028,0009). This also needs careful consideration if non-consecutive frames are requested from an image with non-linearly spaced frames.

Prev | Up | Next
MM.2.2 Start and End Times | Home | MM.2.4 MPEG-2 or MPEG-4 AVC/H.264

DICOM PS3.17 2016c - Explanatory Information