DICOM PS3.17 2016c - Explanatory Information

MM.6 Audio
Prev | MM Considerations For Applications Creating New Images From Multi-frame Images | Next

## MM.6 Audio

Where the original object is MPEG-2 or MPEG-4 AVC/H.264 with interleaved audio data in the MPEG-2 System, and where the retrieved object is also MPEG-2 or MPEG-4 AVC/H.264 encoded, then audio could normally be preserved and maintain synchronization, but in other cases, the audio may be lost.

Prev | Up | Next
MM.5 Time Synchronization | Home | MM.7 Private Attributes

DICOM PS3.17 2016c - Explanatory Information