DICOM PS3.5 2016c - Data Structures and Encoding

A.4.6 MPEG-4 AVC/H.264 HiP@Level4.1 Video Compression
Prev | A.4 Transfer Syntaxes For Encapsulation of Encoded Pixel Data | Next

### A.4.6 MPEG-4 AVC/H.264 HiP@Level4.1 Video Compression

The International Standards Organization ISO/IEC MPEG4 has developed an International Standard, [ISO/IEC 14496-10] (MPEG-4 Part 10), for the video compression of generic coding of moving pictures and associated audio information. This standard is jointly maintained and has identical technical content as the ITU-T H.264 standard.

A DICOM Transfer Syntax for MPEG-4 AVC/H.264 Image Compression shall be identified by a UID value of either:

- 1.2.840.10008.1.2.4.102 corresponding to the MPEG-4 AVC/H.264 High Profile / Level 4.1 of the ITU-T H.264 Video standard

- 1.2.840.10008.1.2.4.103 corresponding to the MPEG-4 AVC/H.264 BD-compatible High Profile / Level 4.1 of the ITU-T H.264 Video standard with the temporal and spatial resolution restrictions defined in Table 8-4.

Prev | Up | Next
A.4.5 MPEG2 Image Compression | Home | A.4.7 MPEG-4 AVC/H.264 HiP@Level4.2 Video Compression

DICOM PS3.5 2016c - Data Structures and Encoding