DICOM PS3.3 2016c - Information Object Definitions

C.8.8.2.2 X-Ray Image Receptor Angle
Prev | C.8.8.2 RT Image Module | Next

##### C.8.8.2.2 X-Ray Image Receptor Angle

The X-Ray Image Receptor Angle (3002,000E) specifies the rotation of the image receptor device in the IEC X-RAY IMAGE RECEPTOR PLANE. A positive angle corresponds to a counter-clockwise rotation of the X-Ray Image Receptor as viewed from the radiation source in the IEC GANTRY coordinate system. The normal (non-rotated) value for this parameter is zero degrees.

Prev | Up | Next
C.8.8.2 RT Image Module | Home | C.8.8.2.3 Image Plane Pixel Spacing and RT Image SID

DICOM PS3.3 2016c - Information Object Definitions