DICOM PS3.3 2016c - Information Object Definitions

A.75.4 Parametric Map IOD Content Constraints
Prev | A.75 Parametric Map IOD | Next

### A.75.4 Parametric Map IOD Content Constraints

Either the Image Pixel Module or the Floating Point Image Pixel Module or the Double Floating Point Image Pixel Module is required, and only one of these shall be present.

### Note

I.e., it is not permitted to have more than one of Pixel Data Provider URL (0028,7FE0), Pixel Data (7FE0,0010), Float Pixel Data (7FE0,0008) or Double Float Pixel Data (7FE0,0009) in a Standard Extended SOP Class in the top level Data Set. See PS3.5.

The VOI LUT Module shall not be present.

The Modality LUT Module shall not be present.

The Overlay Plane Module shall not be present.

The Supplemental Palette Color Lookup Table Module shall not be present.

Prev | Up | Next
A.75.3 Parametric Map IOD Module Table | Home | A.75.5 Parametric Map Functional Groups

DICOM PS3.3 2016c - Information Object Definitions