DICOM PS3.3 2016c - Information Object Definitions

C.8.13.5.7 MR Receive Coil Macro
Prev | C.8.13.5 Enhanced MR Image Functional Group Macros | Next

##### C.8.13.5.7 MR Receive Coil Macro

Table C.8-94 specifies the attributes of the MR Receive Coil Functional Group Macro.

Table C.8-94. MR Receive Coil Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
MR Receive Coil Sequence | (0018,9042) | 1 | A sequence that provides information about each receive coil used. One or more Items shall be included in this Sequence.
>Receive Coil Name | (0018,1250) | 1C | Name of receive coil used. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise.
>Receive Coil Manufacturer Name | (0018,9041) | 2C | Name of manufacturer of receive coil. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise.
>Receive Coil Type | (0018,9043) | 1C | Type of receive coil used. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise. Defined Terms: BODY VOLUME head, extremity, etc. SURFACE MULTICOIL
>Quadrature Receive Coil | (0018,9044) | 1C | Indicates whether the receive coil is quadrature. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise. Enumerated Values: YES quadrature or circularly polarized NO linear
>Multi-Coil Definition Sequence | (0018,9045) | 1C | A sequence that provides information regarding each element of a multi-coil. It should include attributes for all elements, whether used in the current acquisition or not. One or more Items shall be included in this Sequence. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL and Receive Coil Type (0018,9043) equals MULTICOIL. May be present otherwise only if Receive Coil Type (0018,9043) equals MULTICOIL.
>>Multi-Coil Element Name | (0018,9047) | 1 | Name of element of multi-coil.
>>Multi-Coil Element Used | (0018,9048) | 1 | Indicates whether the multi-coil element was used in the current acquisition. Enumerated Values: YES NO
>Multi-Coil Configuration | (0018,9046) | 3 | A textual description of the configuration of multi-coil elements that was used in the current acquisition.

Prev | Up | Next
C.8.13.5.6 MR Imaging Modifier Macro | Home | C.8.13.5.8 MR Transmit Coil Macro

DICOM PS3.3 2016c - Information Object Definitions