DICOM PS3.4 2016c - Service Class Specifications

DD.3.2.3.2 Status
Prev | DD.3.2.3 N-ACTION | Next

##### DD.3.2.3.2 Status

The status values that are specific for these SOP Classes are defined in Table DD.3.2.3-2.

Table DD.3.2.3-2. RT Conventional Machine and RT Ion Machine Verification SOP Class N-ACTION Status Values

Status | Meaning | Code
--- | --- | ---
Success | Machine Parameter Verification of the applicable Machine Verification instance successfully initiated. | 0000
Failure | No such object instance - Machine Verification requested instance not found. | C112

Prev | Up | Next
DD.3.2.3 N-ACTION | Home | DD.3.2.3.3 Behavior

DICOM PS3.4 2016c - Service Class Specifications