DICOM PS3.7 2016c - Message Exchange

C.5.8 Duplicate SOP Instance
Prev | C.5 Failure Status Class | Next

### C.5.8 Duplicate SOP Instance

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0111H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the SOP Instance UID that was already allocated to another SOP Instance.

Prev | Up | Next
C.5.7 Class-Instance Conflict | Home | C.5.9 Duplicate Invocation

DICOM PS3.7 2016c - Message Exchange