DICOM PS3.3 2016c - Information Object Definitions

C.8.13.5.4 MR Echo Macro
Prev | C.8.13.5 Enhanced MR Image Functional Group Macros | Next

##### C.8.13.5.4 MR Echo Macro

Table C.8-91 specifies the attributes of the MR Echo Functional Group Macro.

Table C.8-91. MR Echo Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
MR Echo Sequence | (0018,9114) | 1 | Identifies echo timing of this frame. Only a single Item shall be included in this Sequence.
>Effective Echo Time | (0018,9082) | 1C | The time in ms between the middle of the excitation pulse and the peak of the echo produced for kx=0. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise.

Prev | Up | Next
C.8.13.5.3 MR FOV/Geometry Macro | Home | C.8.13.5.5 MR Modifier Macro

DICOM PS3.3 2016c - Information Object Definitions