DICOM PS3.3 2016c - Information Object Definitions

A.16.2 XRF Image IOD Entity-Relationship Model
Prev | A.16 X-Ray RF Image IOD | Next

### A.16.2 XRF Image IOD Entity-Relationship Model

This IOD uses the E-R Model inSection A.1.2, with only the Image IE below the Series IE.

### Note

When a Study (or Study Component) contains a number of Multi-frame images that do not need to be grouped under different Series, a single Series may be used with a series number containing an arbitrary value (e.g., 1).

Prev | Up | Next
A.16 X-Ray RF Image IOD | Home | A.16.3 XRF Image IOD Module Table

DICOM PS3.3 2016c - Information Object Definitions