DICOM PS3.18 2016c - Web Services

8.2.8 Image Quality
Prev | 8.2 Parameters for DICOM Images | Next

### 8.2.8 Image Quality

The parameter name shall be "imageQuality" for URI based mode, and "ImageQuality" for the WS mode. It is OPTIONAL for the URI based mode and the WS mode "DICOM requester" and "Rendered Requester" transactions. It shall not be present if contentType is application/dicom, except if the transferSyntax parameter is present and corresponds to a lossy compression.

If the requested media type is for a lossy compressed image (e.g., image/jpeg), this parameter indicates the required quality of the image to be returned within the range 1 to 100, 100 being the best quality.

### Note

Decompression and re-compression may degrade the image quality if the original image was already irreversibly compressed. In case the image has been already lossy compressed using the same format as required (e.g., jpeg), it may be sent as it is without decompressing and re-compressing it.

The value shall be encoded as an integer string (IS), as specified in PS3.5.

### Note

The specific interpretation of the meaning of this parameter is left to the interpretation of the implementers of the standard.

Prev | Up | Next
8.2.7 Frame Number | Home | 8.2.9 Unique Identifier of the Presentation Object

DICOM PS3.18 2016c - Web Services