DICOM PS3.3 2016c - Information Object Definitions

A.52.4.2 Overlay Plane Module and VOI LUT Module
Prev | A.52.4 Ophthalmic Tomography Image IOD Content Constraints | Next

#### A.52.4.2 Overlay Plane Module and VOI LUT Module

The Overlay Plane Module and VOI LUT Module shall not be used in a Standard Extended SOP Class of the Ophthalmic Tomography Image.

### Note

In order to annotate images, whether during acquisition or subsequently, SOP Instances of the Grayscale Softcopy Presentation State Storage or the Structured Report Storage SOP Classes that reference the image SOP Instance may be used.

Pseudo-color presentation information may be applied through the use of separate Pseudo-color Softcopy Presentation State SOP instances.

No standard mechanism is provided for inclusion of annotations within the image SOP Instance itself and implementers are discouraged from using private extensions to circumvent this restriction.

Prev | Up | Next
A.52.4 Ophthalmic Tomography Image IOD Content Constraints | Home | A.52.4.3 Ophthalmic Tomography Image Functional Group Macros

DICOM PS3.3 2016c - Information Object Definitions