DICOM PS3.18 2016c - Web Services

8.2.7 Frame Number
Prev | 8.2 Parameters for DICOM Images | Next

### 8.2.7 Frame Number

The parameter name shall be "frameNumber" for URI based mode, and "FrameNumber" for the WS mode.

Specifies that the single frame with that number within a multi-frame image object, as defined in PS3.3 that shall be returned. It is OPTIONAL and shall be ignored in the case of all objects other than multi-frame objects. It shall not be present if contentType is application/dicom.

The value shall be encoded as an integer string (IS), as specified in PS3.5.

Prev | Up | Next
8.2.6 Window Width of the Image | Home | 8.2.8 Image Quality

DICOM PS3.18 2016c - Web Services