DICOM PS3.3 2016c - Information Object Definitions

A.26.5 Acquisition Context Module
Prev | A.26 Digital X-Ray Image IOD | Next

### A.26.5 Acquisition Context Module

The Acquisition Context Module may be used to encode information about conditions present during acquisition that are not described by specific attributes in other modules of the IOD.

The Baseline TID shall be TID 3460 “Projection Radiography Acquisition Context”.

Prev | Up | Next
A.26.4 Overlay Plane Module | Home | A.27 Digital Mammography X-Ray Image IOD

DICOM PS3.3 2016c - Information Object Definitions