DICOM PS3.5 2016c - Data Structures and Encoding

D.3 Examples of Float and Double Float Pixel Data
Prev | D Examples of Various Pixel Data and Overlay Encoding Schemes (Informative) | Next

## D.3 Examples of Float and Double Float Pixel Data

Float Pixel Data having the Value Representation OF always has 32 bits allocated; the resulting byte streams pictured in Figure D.3-1 are as they would be transmitted across a network and/or stored on media.

Figure D.3-1. Sample Float Pixel Data Byte Streams for VR = OF

Double Float Pixel Data having the Value Representation OD always has 64 bits allocated; the resulting byte streams pictured in Figure D.3-2 are as they would be transmitted across a network and/or stored on media.

Figure D.3-2. Sample Float Pixel Data Byte Streams for VR = OD

Prev | Up | Next
D.2 Various Additional Examples of Pixel and Overlay Data Cells | Home | E DICOM Default Character Repertoire (Normative)

DICOM PS3.5 2016c - Data Structures and Encoding