DICOM PS3.17 2016c - Explanatory Information

MM.2.4 MPEG-2 or MPEG-4 AVC/H.264
Prev | MM.2 Frame Extraction Issues | Next

### MM.2.4 MPEG-2 or MPEG-4 AVC/H.264

Identifying the location of the requested frames within an MPEG-2 or MPEG-4 AVC/H.264 data stream is non-trivial, but if achieved, then little else other than changes to the starting times are likely to be required for MPEG-2 or MPEG-4 AVC/H.264 encoded data, as the use-cases for such encoded data (e.g., endoscopy) are unlikely to include explicit frame related data. See the note below however for comments on "single-frame" results.

An application holding data in MPEG-2 or MPEG-4 AVC/H.264 format is unlikely to be able to create a range with a frame increment of greater than one (a calculated frame list with a 3rd value greater than one), and if such a request is made, it might return a status of AA02: Unable to extract Frames.

The approximation feature of the Time Range form of request is especially suitable for data held in MPEG-2 or MPEG-4 AVC/H.264 form, as it allows the application to find the nearest surrounding key frames, which greatly simplifies editing and improves quality.

Prev | Up | Next
MM.2.3 Time Interval versus Frame Increment Vector | Home | MM.2.5 JPEG 2000 Part 2 Multi-Component Transform

DICOM PS3.17 2016c - Explanatory Information