DICOM PS3.4 2016c - Service Class Specifications

B.5 Standard SOP Classes
Prev | B Storage Service Class (Normative) | Next

## B.5 Standard SOP Classes

The SOP Classes in the Storage Service Class identify the Composite IODs to be stored. Table B.5-1 identifies Standard SOP Classes.

Table B.5-1. Standard SOP Classes

SOP Class Name | SOP Class UID | IOD Specification (defined in PS3.3)
--- | --- | ---
Computed Radiography Image Storage | 1.2.840.10008.5.1.4.1.1.1 | Computed Radiography Image IOD
Digital X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.1.1 | Digital X-Ray Image IOD (see Section B.5.1.1)
Digital X-Ray Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.1.1.1 | Digital X-Ray Image IOD (see Section B.5.1.1)
Digital Mammography X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.1.2 | Digital Mammography X-Ray Image IOD (see Section B.5.1.2)
Digital Mammography X-Ray Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.1.2.1 | Digital Mammography X-Ray Image IOD (see Section B.5.1.2)
Digital Intra-Oral X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.1.3 | Digital Intra-Oral X-Ray Image IOD (see Section B.5.1.3)
Digital Intra-Oral X-Ray Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.1.3.1 | Digital Intra-Oral X-Ray Image IOD (see Section B.5.1.3)
CT Image Storage | 1.2.840.10008.5.1.4.1.1.2 | Computed Tomography Image IOD
Enhanced CT Image Storage | 1.2.840.10008.5.1.4.1.1.2.1 | Enhanced CT Image IOD (see Section B.5.1.7)
Legacy Converted Enhanced CT Image Storage | 1.2.840.10008.5.1.4.1.1.2.2 | Legacy Converted Enhanced CT Image IOD (see Section B.5.1.7)
Ultrasound Multi-frame Image Storage | 1.2.840.10008.5.1.4.1.1.3.1 | Ultrasound Multi-frame Image IOD
MR Image Storage | 1.2.840.10008.5.1.4.1.1.4 | Magnetic Resonance Image IOD
Enhanced MR Image Storage | 1.2.840.10008.5.1.4.1.1.4.1 | Enhanced MR Image IOD (see Section B.5.1.6)
MR Spectroscopy Storage | 1.2.840.10008.5.1.4.1.1.4.2 | MR Spectroscopy IOD
Enhanced MR Color Image Storage | 1.2.840.10008.5.1.4.1.1.4.3 | Enhanced MR Color Image IOD
Legacy Converted Enhanced MR Image Storage | 1.2.840.10008.5.1.4.1.1.4.4 | Legacy Converted Enhanced MR Image IOD (see Section B.5.1.6)
Ultrasound Image Storage | 1.2.840.10008.5.1.4.1.1.6.1 | Ultrasound Image IOD
Enhanced US Volume Storage | 1.2.840.10008.5.1.4.1.1.6.2 | Enhanced US Volume IOD
Secondary Capture Image Storage | 1.2.840.10008.5.1.4.1.1.7 | Secondary Capture Image IOD
Multi-frame Single Bit Secondary Capture Image Storage | 1.2.840.10008.5.1.4.1.1.7.1 | Multi-frame Single Bit Secondary Capture Image IOD
Multi-frame Grayscale Byte Secondary Capture Image Storage | 1.2.840.10008.5.1.4.1.1.7.2 | Multi-frame Grayscale Byte Secondary Capture Image IOD
Multi-frame Grayscale Word Secondary Capture Image Storage | 1.2.840.10008.5.1.4.1.1.7.3 | Multi-frame Grayscale Word Secondary Capture Image IOD
Multi-frame True Color Secondary Capture Image Storage | 1.2.840.10008.5.1.4.1.1.7.4 | Multi-frame True Color Secondary Capture Image IOD
12-lead ECG Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.1.1 | 12-Lead Electrocardiogram IOD
General ECG Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.1.2 | General Electrocardiogram IOD
Ambulatory ECG Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.1.3 | Ambulatory Electrocardiogram IOD
Hemodynamic Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.2.1 | Hemodynamic IOD
Cardiac Electrophysiology Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.3.1 | Basic Cardiac Electrophysiology IOD
Basic Voice Audio Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.4.1 | Basic Voice Audio IOD
General Audio Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.4.2 | General Audio Waveform IOD
Arterial Pulse Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.5.1 | Arterial Pulse Waveform IOD
Respiratory Waveform Storage | 1.2.840.10008.5.1.4.1.1.9.6.1 | Respiratory Waveform IOD
Grayscale Softcopy Presentation State Storage | 1.2.840.10008.5.1.4.1.1.11.1 | Grayscale Softcopy Presentation State IOD
Color Softcopy Presentation State Storage | 1.2.840.10008.5.1.4.1.1.11.2 | Color Softcopy Presentation State IOD
Pseudo-Color Softcopy Presentation State Storage | 1.2.840.10008.5.1.4.1.1.11.3 | Pseudo-color Softcopy Presentation State IOD
Blending Softcopy Presentation State Storage | 1.2.840.10008.5.1.4.1.1.11.4 | Blending Softcopy Presentation State IOD
XA/XRF Grayscale Softcopy Presentation State Storage | 1.2.840.10008.5.1.4.1.1.11.5 | XA/XRF Grayscale Softcopy Presentation State IOD
Grayscale Planar MPR Volumetric Presentation State Storage | 1.2.840.10008.​5.​1.​4.​1.​1.​11.​6 | Planar MPR Volumetric Presentation State IOD Description
Compositing Planar MPR Volumetric Presentation State Storage | 1.2.840.10008.​5.​1.​4.​1.​1.​11.​7 | Planar MPR Volumetric Presentation State IOD Description
X-Ray Angiographic Image Storage | 1.2.840.10008.5.1.4.1.1.12.1 | X-Ray Angiographic Image IOD
Enhanced XA Image Storage | 1.2.840.10008.5.1.4.1.1.12.1.1 | Enhanced X-Ray Angiographic Image IOD
X-Ray Radiofluoroscopic Image Storage | 1.2.840.10008.5.1.4.1.1.12.2 | X-Ray RF Image IOD
Enhanced XRF Image Storage | 1.2.840.10008.5.1.4.1.1.12.2.1 | Enhanced X-Ray RF Image IOD
X-Ray 3D Angiographic Image Storage | 1.2.840.10008.5.1.4.1.1.13.1.1 | X-Ray 3D Angiographic Image IOD
X-Ray 3D Craniofacial Image Storage | 1.2.840.10008.5.1.4.1.1.13.1.2 | X-Ray 3D Craniofacial Image IOD
Breast Tomosynthesis Image Storage | 1.2.840.10008.5.1.4.1.1.13.1.3 | Breast Tomosynthesis Image IOD
Breast Projection X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.13.1.4 | Breast Projection X-Ray Image IOD
Breast Projection X-Ray Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.13.1.5 | Breast Projection X-Ray Image IOD
Intravascular Optical Coherence Tomography Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.14.1 | Intravascular OCT IOD (see Section B.5.1.13)
Intravascular Optical Coherence Tomography Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.14.2 | Intravascular OCT IOD (see Section B.5.1.13)
Nuclear Medicine Image Storage | 1.2.840.10008.5.1.4.1.1.20 | Nuclear Medicine Image IOD
Parametric Map Storage | 1.2.840.10008.5.1.4.1.1.30 | Parametric Map IOD
Raw Data Storage | 1.2.840.10008.5.1.4.1.1.66 | Raw Data IOD
Spatial Registration Storage | 1.2.840.10008.5.1.4.1.1.66.1 | Spatial Registration IOD
Spatial Fiducials Storage | 1.2.840.10008.5.1.4.1.1.66.2 | Spatial Fiducials IOD
Deformable Spatial Registration Storage | 1.2.840.10008.5.1.4.1.1.66.3 | Deformable Spatial Registration IOD
Segmentation Storage | 1.2.840.10008.5.1.4.1.1.66.4 | Segmentation IOD
Surface Segmentation Storage | 1.2.840.10008.5.1.4.1.1.66.5 | Surface Segmentation IOD
Tractography Results Storage | 1.2.840.10008.5.1.4.1.1.66.6 | Tractography Results IOD
Real World Value Mapping Storage | 1.2.840.10008.5.1.4.1.1.67 | Real World Value Mapping IOD
Surface Scan Mesh Storage | 1.2.840.10008.5.1.4.1.1.68.1 | Surface Scan Mesh IOD
Surface Scan Point Cloud Storage | 1.2.840.10008.5.1.4.1.1.68.2 | Surface Scan Point Cloud IOD
VL Endoscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.1 | VL Endoscopic Image IOD
Video Endoscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.1.1 | Video Endoscopic Image IOD
VL Microscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.2 | VL Microscopic Image IOD
Video Microscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.2.1 | Video Microscopic Image IOD
VL Slide-Coordinates Microscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.3 | VL Slide-coordinates Microscopic Image IOD
VL Photographic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.4 | VL Photographic Image IOD
Video Photographic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.4.1 | Video Photographic Image IOD
Ophthalmic Photography 8 Bit Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.5.1 | Ophthalmic Photography 8 Bit Image IOD
Ophthalmic Photography 16 Bit Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.5.2 | Ophthalmic Photography 16 Bit Image IOD
Stereometric Relationship Storage | 1.2.840.10008.5.1.4.1.1.77.1.5.3 | Stereometric Relationship IOD
Ophthalmic Tomography Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.5.4 | Ophthalmic Tomography Image IOD
Wide Field Ophthalmic Photography Stereographic Projection Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.5.5 | Wide Field Ophthalmic Photography Stereographic Projection Image IOD
Wide Field Ophthalmic Photography 3D Coordinates Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.5.6 | Wide Field Ophthalmic Photography 3D Coordinates Image IOD
VL Whole Slide Microscopy Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.6 | VL Whole Slide Microscopy Image IOD
Lensometry Measurements Storage | 1.2.840.10008.5.1.4.1.1.78.1 | Lensometry Measurements IOD
Autorefraction Measurements Storage | 1.2.840.10008.5.1.4.1.1.78.2 | Autorefraction Measurements IOD
Keratometry Measurements Storage | 1.2.840.10008.5.1.4.1.1.78.3 | Keratometry Measurements IOD
Subjective Refraction Measurements Storage | 1.2.840.10008.5.1.4.1.1.78.4 | Subjective Refraction Measurements IOD
Visual Acuity Measurements Storage | 1.2.840.10008.5.1.4.1.1.78.5 | Visual Acuity Measurements IOD
Spectacle Prescription Report Storage | 1.2.840.10008.5.1.4.1.1.78.6 | Spectacle Prescription Report IOD
Ophthalmic Axial Measurements Storage | 1.2.840.10008.5.1.4.1.1.78.7 | Ophthalmic Axial Measurements IOD
Intraocular Lens Calculations Storage | 1.2.840.10008.5.1.4.1.1.78.8 | Intraocular Lens Calculations IOD
Macular Grid Thickness and Volume Report | 1.2.840.10008.5.1.4.1.1.79.1 | Macular Grid Thickness and Volume Report IOD
Ophthalmic Visual Field Static Perimetry Measurements Storage | 1.2.840.10008.5.1.4.1.1.80.1 | Ophthalmic Visual Field Static Perimetry Measurements IOD
Ophthalmic Thickness Map Storage | 1.2.840.10008.5.1.4.1.1.81.1 | Ophthalmic Thickness Map IOD
Corneal Topography Map Storage | 1.2.840.10008.5.1.4.1.1.82.1 | Corneal Topography Map IOD
Basic Text SR Storage | 1.2.840.10008.5.1.4.1.1.88.11 | Basic Text SR IOD
Enhanced SR Storage | 1.2.840.10008.5.1.4.1.1.88.22 | Enhanced SR IOD
Comprehensive SR Storage | 1.2.840.10008.5.1.4.1.1.88.33 | Comprehensive SR IOD
Comprehensive 3D SR Storage | 1.2.840.10008.5.1.4.1.1.88.34 | Comprehensive 3D SR IOD
Extensible SR Storage | 1.2.840.10008.5.1.4.1.1.88.35 | Extensible SR IOD
Procedure Log Storage | 1.2.840.10008.5.1.4.1.1.88.40 | Procedure Log IOD
Mammography CAD SR Storage | 1.2.840.10008.5.1.4.1.1.88.50 | Mammography CAD SR IOD
Key Object Selection Storage | 1.2.840.10008.5.1.4.1.1.88.59 | Key Object Selection Document IOD
Chest CAD SR Storage | 1.2.840.10008.5.1.4.1.1.88.65 | Chest CAD SR IOD
X-Ray Radiation Dose SR Storage | 1.2.840.10008.5.1.4.1.1.88.67 | X-Ray Radiation Dose SR IOD
Radiopharmaceutical Radiation Dose SR Storage | 1.2.840.10008.5.1.4.1.1.88.68 | Radiopharmaceutical Radiation Dose SR IOD
Colon CAD SR Storage | 1.2.840.10008.5.1.4.1.1.88.69 | Colon CAD SR IOD
Implantation Plan SR Document Storage | 1.2.840.10008.5.1.4.1.1.88.70 | Implantation Plan SR Document IOD
Acquisition Context SR Storage | 1.2.840.10008.5.​1.​4.​1.​1.​88.​71 | Acquisition Context SR IOD
Content Assessment Results Storage | 1.2.840.10008.5.1.4.1.1.90.1 | Content Assessment Results IOD
Encapsulated PDF Storage | 1.2.840.10008.5.1.4.1.1.104.1 | Encapsulated PDF IOD
Encapsulated CDA Storage | 1.2.840.10008.5.1.4.1.1.104.2 | Encapsulated CDA IOD
Positron Emission Tomography Image Storage | 1.2.840.10008.5.1.4.1.1.128 | Positron Emission Tomography Image IOD
Enhanced PET Image Storage | 1.2.840.10008.5.1.4.1.1.130 | Enhanced PET Image IOD (see Section B.5.1.16)
Legacy Converted Enhanced PET Image Storage | 1.2.840.10008.5.1.4.1.1.128.1 | Legacy Converted Enhanced PET Image IOD
Basic Structured Display Storage | 1.2.840.10008.5.1.4.1.1.131 | Basic Structured Display IOD
RT Image Storage | 1.2.840.10008.5.1.4.1.1.481.1 | RT Image IOD
RT Dose Storage | 1.2.840.10008.5.1.4.1.1.481.2 | RT Dose IOD
RT Structure Set Storage | 1.2.840.10008.5.1.4.1.1.481.3 | RT Structure Set IOD
RT Beams Treatment Record Storage | 1.2.840.10008.5.1.4.1.1.481.4 | RT Beams Treatment Record IOD
RT Plan Storage | 1.2.840.10008.5.1.4.1.1.481.5 | RT Plan IOD
RT Brachy Treatment Record Storage | 1.2.840.10008.5.1.4.1.1.481.6 | RT Brachy Treatment Record IOD
RT Treatment Summary Record Storage | 1.2.840.10008.5.1.4.1.1.481.7 | RT Treatment Summary Record IOD
RT Ion Plan Storage | 1.2.840.10008.5.1.4.1.1.481.8 | RT Ion Plan IOD
RT Ion Beams Treatment Record Storage | 1.2.840.10008.5.1.4.1.1.481.9 | RT Ion Beams Treatment Record IOD
RT Beams Delivery Instruction Storage | 1.2.840.10008.5.1.4.34.7 | RT Beams Delivery Instruction IOD
RT Brachy Application Setup Delivery Instruction Storage | 1.2.840.10008.5.1.4.34.10 | RT Brachy Application Setup Delivery Instruction IOD

### Note

The Generic Implant Template Storage, Implant Assembly Template Storage, and Implant Template Group Storage SOP Classes were formerly specified in this table, incorrectly since they do not use the Patient / Study / Series / Instance information model. Those have been consolidated into the Non-Patient Object Storage Service Class (see Annex GG).

### B.5.1 Specialization for Standard SOP Classes

#### B.5.1.1 Digital X-Ray Image Storage SOP Classes

The Digital X-Ray Image Storage - For Presentation SOP Class shall use the DX IOD with an Enumerated Value of FOR PRESENTATION for Presentation Intent Type (0008,0068).

The Digital X-Ray Image Storage - For Processing SOP Class shall use the DX IOD with an Enumerated Value of FOR PROCESSING for Presentation Intent Type (0008,0068).

An SCU or SCP of the Digital X-Ray Image Storage - For Processing SOP Class shall also support the Digital X-Ray Image Storage - For Presentation SOP Class.

### Note

1. The intent of this requirement is to ensure a useful level of interoperability by avoiding the situation where an SCU might support only the Digital X-Ray Image Storage - For Processing SOP Class and an SCP only the Digital X-Ray Image Storage - For Presentation SOP Class, or vice versa. The burden is therefore to support the Digital X-Ray Image Storage - For Presentation SOP Class as a "baseline".

2. The term "support" is used in this section in the sense that an SCU or SCP must be capable of sending or receiving the For Presentation SOP Class. There is no intent to imply that an SCU must always send an instance of the For Presentation SOP Class when an instance of the For Processing SOP Class is sent.

   Nor is there any intent to imply that during Association establishment, that a Presentation Context for the For Presentation SOP Class has to be proposed by the initiator. However, an association acceptor may reject a For Presentation SOP Class Presentation Context if it accepts a For Processing SOP Class Presentation Context, and prefers that SOP Class, in which case it may no longer be able to "pass on" the object later as an SCU unless it is able to generate a For Presentation object.

   It is not possible for an SCP to determine from proposed Presentation Contexts whether or not an SCU "supports" (is capable of sending) both For Processing and For Presentation SOP Class Instances. Such a determination requires a priori knowledge of the information contained in the Conformance Statement for the SCU, as well as how the SCU is configured and operated. An SCU that supports both SOP Classes may well choose to only propose one or the other during Association establishment, depending on which Instances it actually intends to send over that particular association (although the SCU must be capable of sending instances of the For Presentation SOP Class if the SCP does not accept the For Processing).

   The intent of the requirement is that if an SCU is only capable of sending the For Presentation SOP Class, any SCP will be guaranteed to be able to receive it. Conversely, if an SCP is only capable of receiving the For Presentation SOP Class, any SCU will be guaranteed to be able to send it.

#### B.5.1.2 Digital Mammography X-Ray Image Storage SOP Classes

The Digital Mammography X-Ray Image Storage - For Presentation SOP Class shall use the Digital Mammography IOD with an Enumerated Value of FOR PRESENTATION for Presentation Intent Type (0008,0068).

The Digital Mammography X-Ray Image Storage - For Processing SOP Class shall use the Digital Mammography IOD with an Enumerated Value of FOR PROCESSING for Presentation Intent Type (0008,0068).

An SCU or SCP of the Digital Mammography X-Ray Image Storage - For Processing SOP Class shall also support the Digital Mammography X-Ray Image Storage - For Presentation SOP Class.

#### B.5.1.3 Digital Intra-Oral X-Ray Image Storage SOP Classes

The Digital Intra-Oral X-Ray Image Storage - For Presentation SOP Class shall use the Digital Intra-Oral X-Ray IOD with an Enumerated Value of FOR PRESENTATION for Presentation Intent Type (0008,0068).

The Digital Intra-Oral X-Ray Image Storage - For Processing SOP Class shall use the Digital Intra-Oral X-Ray IOD with an Enumerated Value of FOR PROCESSING for Presentation Intent Type (0008,0068).

An SCU or SCP of the Digital Intra-Oral X-Ray Image Storage - For Processing SOP Class shall also support the Digital Intra-Oral X-Ray Image Storage - For Presentation SOP Class.

#### B.5.1.4 Softcopy Presentation State Storage SOP Classes

See Annex N.

#### B.5.1.5 Structured Reporting Storage SOP Classes

The requirements of Annex O apply to the following SOP Classes:

- Basic Text SR

- Extensible SR, Enhanced SR, and SOP Classes for which it is the Related General SOP Class

- Comprehensive 3D SR, Comprehensive SR, and SOP Classes for which they are the Related General SOP Classes

- Mammography CAD SR

- Chest CAD SR

- Procedure Log

- X-Ray Radiation Dose SR

- Radiopharmaceutical Radiation Dose SR

- Spectacle Prescription Report

- Colon CAD SR

- Macular Grid Thickness and Volume Report

- Implantation Plan SR Document

- Acquisition Context SR

Annex O requirements do not apply to the Key Object Selection Document SOP Class.

#### B.5.1.6 Enhanced MR Image Storage and Legacy Converted Enhanced MR Image Storage SOP Class

An SCP of the Enhanced MR Image Storage or Legacy Converted Enhanced MR Image Storage SOP Class shall also support the Grayscale Softcopy Presentation State Storage SOP Class.

### Note

This requirement is present in order to allow the exchange of graphical annotations created by an acquisition or conversion device.

#### B.5.1.7 Enhanced CT Image Storage and Legacy Converted Enhanced CT Image Storage SOP Class

An SCP of the Enhanced CT Image Storage or Legacy Converted Enhanced CT Image Storage SOP Class shall also support the Grayscale Softcopy Presentation State Storage SOP Class.

### Note

This requirement is present in order to allow the exchange of graphical annotations created by an acquisition or conversion device.

#### B.5.1.8 Enhanced MR Color Image Storage SOP Class

An SCP of the Enhanced MR Color Image Storage SOP Class shall also support the Color Softcopy Presentation State Storage SOP Class.

### Note

This requirement is present in order to allow the exchange of graphical annotations created by an acquisition device.

#### B.5.1.9 Basic Structured Display

An SCU of the Basic Structured Display Storage SOP Class that creates SOP Instances of the Class shall identify in its Conformance Statement the Composite Storage SOP Classes and Softcopy Presentation State Storage SOP Classes that are also supported by the SCU, and may be referenced by Basic Structured Display SOP Instances it creates. It shall identify in its Conformance Statement the values it may use in the Attributes Image Box Layout Type (0072,0304) and Type of Synchronization (0072,0434).

An SCP of the Basic Structured Display Storage SOP Class, when rendering SOP Instances of the Class, shall preserve the aspect ratio specified by the Nominal Screen Definition Sequence (0072,0102) Attributes Number of Vertical Pixels (0072,0104) and Number of Horizontal Pixels (0072,0106) without clipping.

### Note

1. The SCP is not required to display using the exact number of vertical and horizontal pixels. The SCP may use as much of its display screen as it desires, while maintaining the Structured Display aspect ratio.

2. If the display screen has a different aspect ratio, the positioning of the display on the screen is unspecified (centered, left or right justified, top or bottom justified).

An SCP of the Basic Structured Display Storage SOP Class that is capable of rendering SOP Instances of the Class shall identify in its Conformance Statement the Composite Storage SOP Classes and Softcopy Presentation State Storage SOP Classes that are also supported by the SCP, and will be rendered when referenced by Basic Structured Display SOP Instances for display. It shall specify in its Conformance Statement the user display controls and interactions for the values of Image Box Layout Type (0072,0304) and Type of Synchronization (0072,0434) that it supports. It shall identify in its Conformance Statement its behavior when encountering a referenced Presentation State or other Composite Storage SOP Instance whose display it does not support, or an unsupported value of Image Box Layout Type or Type of Synchronization; such behavior shall include at a minimum a display to the user of the nature of the incompatibility.

#### B.5.1.10 Implant Template Storage SOP Classes

See Annex GG.

### Note

The requirements of this section have been consolidated into the Non-Patient Object Storage Service Class (see Section GG.6.3).

#### B.5.1.11 Ophthalmic Axial Measurements Storage SOP Class

Ophthalmic axial measurements devices are used in the preoperative assessment of every cataract surgery patient. Ophthalmic axial measurements SOP Classes support ophthalmic axial measurements devices.

For a device that is both a SCU and a SCP of the Ophthalmic Axial Measurements Storage SOP Class, in addition to the behavior for the Storage Service Class specified in Section B.2.2, the following additional requirements are specified for Ophthalmic Axial Measurements Storage SOP Classes:

- A SCP of this SOP Class shall support Level 2 Conformance as defined in Section B.4.1.

### Note

This requirement means that all Type 1, Type 2, and Type 3 Attributes defined in the Information Object Definition and Private Attributes associated with the SOP Class will be stored and may be accessed.

#### B.5.1.12 IOL Calculation Storage SOP Class

IOL (intraocular lens) calculation is used in the preoperative assessment of every cataract surgery patient. IOL Calculation SOP Classes support IOL calculation software, which may be located either on ophthalmic axial measurement devices or on a separate computer.

For a device that is both a SCU and a SCP of the IOL Calculation Storage SOP Class, in addition to the behavior for the Storage Service Class specified in Section B.2.2, the following additional requirements are specified for IOL Calculation Storage SOP Classes:

- A SCP of this SOP Class shall support Level 2 Conformance as defined in Section B.4.1.

### Note

This requirement means that all Type 1, Type 2, and Type 3 Attributes defined in the Information Object Definition and Private Attributes associated with the SOP Class will be stored and may be accessed.

#### B.5.1.13 Intravascular OCT Image Storage SOP Classes

The Intravascular OCT Image Storage - For Presentation SOP Class shall use the IVOCT IOD with an Enumerated Value of FOR PRESENTATION for Presentation Intent Type (0008,0068).

The Intravascular OCT Image Storage - For Processing SOP Class shall use the IVOCT IOD with an Enumerated Value of FOR PROCESSING for Presentation Intent Type (0008,0068).

An SCU or SCP of the Intravascular OCT Image Storage - For Processing SOP Class shall also support the Intravascular OCT Image Storage - For Presentation SOP Class.

### Note

1. The intent of this requirement is to ensure a useful level of interoperability by avoiding the situation where an SCU might support only the Intravascular OCT Image Storage - For Processing SOP Class and an SCP only the Intravascular OCT Image Storage - For Presentation SOP Class, or vice versa. The burden is therefore to support the Intravascular OCT Image Storage - For Presentation SOP Class as a "baseline".

2. The term "support" is used in this section in the sense that an SCU or SCP must be capable of sending or receiving the For Presentation SOP Class. There is no intent to imply that an SCU must always send an instance of the For Presentation SOP Class when an instance of the For Processing SOP Class is sent.

   Nor is there any intent to imply that during Association establishment, that a Presentation Context for the For Presentation SOP Class has to be proposed by the initiator. However, an association acceptor may reject a For Presentation SOP Class Presentation Context if it accepts a For Processing SOP Class Presentation Context, and prefers that SOP Class, in which case it may no longer be able to "pass on" the object later as an SCU unless it is able to generate a For Presentation object.

   It is not possible for an SCP to determine from proposed Presentation Contexts whether or not an SCU "supports" (is capable of sending) both For Processing and For Presentation SOP Class Instances. Such a determination requires a priori knowledge of the information contained in the Conformance Statement for the SCU, as well as how the SCU is configured and operated. An SCU that supports both SOP Classes may well choose to only propose one or the other during Association establishment, depending on which Instances it actually intends to send over that particular association (although the SCU must be capable of sending instances of the For Presentation SOP Class if the SCP does not accept the For Processing).

   The intent of the requirement is that if an SCU is only capable of sending the For Presentation SOP Class, any SCP will be guaranteed to be able to receive it. Conversely, if an SCP is only capable of receiving the For Presentation SOP Class, any SCU will be guaranteed to be able to send it.

#### B.5.1.14 Ophthalmic Thickness Map Storage SOP Class

The Ophthalmic Thickness Map SOP Class encodes a topographic representation of the thickness/height measurements of the posterior eye.

For a device that is both a SCU and a SCP of the Ophthalmic Thickness Map Storage SOP Class, in addition to the behavior for the Storage Service Class specified in Section B.2.2, the following additional requirements are specified for Ophthalmic Thickness Map Storage SOP Classes:

- A SCP of this SOP Class shall support Level 2 Conformance as defined in Section B.4.1.

### Note

This requirement means that all Type 1, Type 2, and Type 3 Attributes defined in the Information Object Definition and Private Attributes associated with the SOP Class will be stored and may be accessed.

#### B.5.1.15 Enhanced PET Image Storage and Legacy Converted Enhanced PET Image Storage SOP Class

An SCP of the Enhanced PET Image Storage or Legacy Converted Enhanced PET Image Storage SOP Class shall also support the Grayscale Softcopy Presentation State Storage SOP Class.

### Note

This requirement is present in order to allow the exchange of graphical annotations created by an acquisition or conversion device.

#### B.5.1.16 Enhanced PET Image Storage SOP Classes

An SCP of the Enhanced PET Image Storage SOP Class shall also support the Grayscale Softcopy Presentation State Storage SOP Class.

### Note

This requirement is present in order to allow the exchange of graphical annotations created by an acquisition device.

#### B.5.1.17 Corneal Topography Map Storage SOP Class

The Corneal Topography Map SOP Class encodes a topographic representation of the curvature and/or elevation measurements of corneal anterior and posterior surfaces (e.g., maps that display corneal curvatures, corneal elevations, and corneal power, etc.).

For a device that is both a SCU and a SCP of the Corneal Topography Map Storage SOP Class, in addition to the behavior for the Storage Service Class specified in Section B.2.2, the following additional requirements are specified for Corneal Topography Map Storage SOP Classes:

- A SCP of this SOP Class shall support Level 2 Conformance as defined in Section B.4.1.

### Note

This requirement means that all Type 1, Type 2, and Type 3 Attributes defined in the Information Object Definition and Private Attributes associated with the SOP Class will be stored and may be accessed.

#### B.5.1.18 Breast Projection X-Ray Image Storage SOP Classes

The Breast Projection X-Ray Image Storage - For Presentation SOP Class shall use the Breast Projection X-Ray Image IOD with an Enumerated Value of FOR PRESENTATION for Presentation Intent Type (0008,0068).

The Breast Projection X-Ray Image Storage - For Processing SOP Class shall use the Breast Projection X-Ray Image IOD with an Enumerated Value of FOR PROCESSING for Presentation Intent Type (0008,0068).

An SCU or SCP of the Breast Projection X-Ray Image Storage - For Processing SOP Class shall also support the Breast Projection X-Ray Image Storage - For Presentation SOP Class.

#### B.5.1.19 Planar MPR Volumetric Presentation State Storage SOP Classes

The requirements of Annex FF apply to the following SOP Classes:

- Grayscale Planar MPR Volumetric Presentation State Storage

- Compositing Planar MPR Volumetric Presentation State Storage

The Grayscale Planar MPR Volumetric Presentation State Storage SOP Class shall use the Planar MPR Volumetric Presentation State IOD with an Enumerated Value of MONOCHROME for Pixel Presentation (0008,9205) and shall have only a single item in the Volumetric Presentation State Input Sequence (0070,1201).

The Compositing Planar MPR Volumetric Presentation State Storage SOP Class shall use the Planar MPR Volumetric Presentation State IOD with an Enumerated Value of TRUE COLOR for Pixel Presentation (0008,9205).

#### B.5.1.20 Content Assessment Results Storage SOP Classes

An SCU of the Content Assessment Results Storage SOP Class that creates SOP Instances of the Class shall identify in its Conformance Statement the criteria for setting the Observation Significance (0082,0008).

Prev | Up | Next
B.4.4.2 Specialized Information Object Definition | Home | B.6 Retired Standard SOP Classes

DICOM PS3.4 2016c - Service Class Specifications