DICOM PS3.17 2016c - Explanatory Information

UUU.1.3 Introduction to 2D to 3D Map For Wide Field Ophthalmic Photography
Prev | UUU Ophthalmology Use Cases (Informative) | Next

## UUU.1.3 Introduction to 2D to 3D Map For Wide Field Ophthalmic Photography

A 2D to 3D map includes 3D coordinates of all or a subset of pixels (namely coordinate points) to the 2D image. Implementations choose the interpolation type used, but it is recommended to use a spline based interpolation. See Figure UUU.1.3-1.

Pixels' 3D coordinates could be used for different analyses and computations e.g. measuring the length of a path, and calculating the area of region of interest, 3D computer graphics, registration, shortest distance computation, etc. Some examples of methods using 3D coordinates are listed in the following subsections.

Figure UUU.1.3-1. Map pixel to 3D coordinate

### UUU.1.3.1 Measuring the Length of a Path

Let the path between points A, and B be represented by set of N following pixels P={pi} and p0=A and pN=B. The length of this path can be computed from the partial lengths between path points by:

where:

and where xi, yi, zi are the 3D coordinates of the point pi which is either available in the 2D to 3D map if pi is a coordinate point or it is computed by interpolation. Here it is assumed that the sequence of path points is known and the path is 4- or 8-connected (i.e., the path points are neighbors with no more than one pixel distance in horizontal, vertical, or diagonal direction). It is recommendable to support sub-pixel processing by using interpolation.

Figure UUU.1.3-2. Measure the Length of a Path

Prev | Up | Next
UUU Ophthalmology Use Cases (Informative) | Home | UUU.1.3.2 Shortest Distance Between Two Points

DICOM PS3.17 2016c - Explanatory Information