DICOM PS3.3 2016c - Information Object Definitions

A.16.3 XRF Image IOD Module Table
Prev | A.16 X-Ray RF Image IOD | Next

### A.16.3 XRF Image IOD Module Table

Table A.16-1 specifies the Modules of the XRF Image IOD.

Table A.16-1. XRF Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Synchronization | C.7.4.2 | U
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
Image Pixel | C.7.6.3 | M
Contrast/Bolus | C.7.6.4 | C - Required if contrast media was used in this Image
Cine | C.7.6.5 | C - Required if pixel data is Multi-frame Cine Data
Multi-frame | C.7.6.6 | C - Required if pixel data is Multi-frame Cine Data
Frame Pointers | C.7.6.9 | U
Mask | C.7.6.10 | C - Required if the Image may be subtracted
Display Shutter | C.7.6.11 | U
Device | C.7.6.12 | U
Intervention | C.7.6.13 | U
Specimen | C.7.6.22 | U
X-Ray Image | C.8.7.1 | M
X-Ray Acquisition | C.8.7.2 | M
X-Ray Collimator | C.8.7.3 | U
X-Ray Table | C.8.7.4 | U
XRF Positioner | C.8.7.6 | U
X-Ray Tomography Acquisition | C.8.7.7 | C - Required if Scan Option (0018,0022) is TOMO
DX Detector | C.8.11.4 | U
Overlay Plane | C.9.2 | U
Multi-frame Overlay | C.9.3 | C - Required if Overlay Data contains multiple frames
Modality LUT | C.11.1 | C - Required if Pixel Intensity Relationship (0028,1040) is LOG U - Optional if Pixel Intensity Relationship (0028,1040) is DISP
VOI LUT | C.11.2 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

### Note

The Curve Module (Retired) was previously included in the Image IE for this IOD but has been retired. See PS3.3-2004.

Prev | Up | Next
A.16.2 XRF Image IOD Entity-Relationship Model | Home | A.17 RT Image IOD

DICOM PS3.3 2016c - Information Object Definitions