DICOM PS3.4 2016c - Service Class Specifications

J.3 Storage Commitment Push Model SOP Class
Prev | J Storage Commitment Service Class (Normative) | Next

## J.3 Storage Commitment Push Model SOP Class

The Storage Commitment Push Model SOP Class is intended for those Application Entities requiring storage commitment where the SCU determines the time at which the SOP Instances are transmitted. The SCU transmits the SOP Instances to the SCP using an appropriate mechanism. The request for storage commitment is transmitted to the SCP together with a list of references to one or more SOP Instances. Success or failure of storage commitment is subsequently indicated by a notification from the SCP to the SCU.

### J.3.1 DIMSE Service Group

The DIMSE-N Services applicable to the Storage Commitment Push Model SOP Class are shown in Table J.3.1-1.

Table J.3.1-1. IOD DIMSE Services

DIMSE Service Element | Usage SCU/SCP
--- | ---
N-EVENT-REPORT | M/M
N-ACTION | M/M

The DIMSE-N Services and Protocol are specified in PS3.7.

Prev | Up | Next
J.2 Conformance Overview | Home | J.3.2 Operations

DICOM PS3.4 2016c - Service Class Specifications