DICOM PS3.3 2016c - Information Object Definitions

C.8.19.6.8 X-Ray Frame Acquisition Macro
Prev | C.8.19.6 Enhanced XA/XRF Image Functional Group Macros | Next

##### C.8.19.6.8 X-Ray Frame Acquisition Macro

Table C.8.19.6-8 specifies the attributes containing the X-Ray Frame Acquisition Functional Group Macro.

Table C.8.19.6-8. X-Ray Frame Acquisition Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Frame Acquisition Sequence | (0018,9417) | 1 | Sequence containing the acquisition parameters for this frame. Only a single Item shall be included in this Sequence.
>KVP | (0018,0060) | 1 | Exact peak kilo voltage output of the X-Ray generator used for this frame.
>X-Ray Tube Current in mA | (0018,9330) | 1 | Exact Nominal X-Ray tube current in milliamperes applied during Acquisition Duration (0018,9220) for this frame.

###### C.8.19.6.8.1 X-Ray Frame Acquisition Sequence Attributes

These attribute may only be used if the information is available on a frame-by-frame base. The average values for these attributes of all frames shall be stored in the same attribute in the XA/XRF Acquisition Module.

Prev | Up | Next
C.8.19.6.7 X-Ray Object Thickness Macro | Home | C.8.19.6.9 X-Ray Projection Pixel Calibration Macro

DICOM PS3.3 2016c - Information Object Definitions