DICOM PS3.17 2016c - Explanatory Information

S.5.2 NTP
Prev | S.5 Adding The First Managed Device to A Legacy Network | Next

### S.5.2 NTP

The NTP server location relative to this device should be reviewed to be sure that it meets the timing requirements of the device. If it is an NTP client with a time accuracy requirement of approximately 1 second, almost any NTP server location will be acceptable. For SNTP clients and devices with high time accuracy requirements, it is possible that an additional NTP server or network topology adjustment may be needed.

If the NTP server is using secured time information, certificates or passwords may need to be exchanged.

Prev | Up | Next
S.5 Adding The First Managed Device to A Legacy Network | Home | S.5.3 Documenting Managed and Unmanaged Nodes (DHCP, DNS, and LDAP)

DICOM PS3.17 2016c - Explanatory Information