DICOM PS3.7 2016c - Message Exchange

C.5.9 Duplicate Invocation
Prev | C.5 Failure Status Class | Next

### C.5.9 Duplicate Invocation

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0210H.

Prev | Up | Next
C.5.8 Duplicate SOP Instance | Home | C.5.10 Invalid Argument Value

DICOM PS3.7 2016c - Message Exchange