DICOM PS3.2 2016c - Conformance

I.4.4.3 RS Interface
Prev | I.4.4 Configuration | Next

#### I.4.4.3 RS Interface

The EXAMPLE-WADO-SERVICE can be configured to respond on two ports, one for unprotected HTTP traffic and one for TLS protected traffic. The TLS port will refuse any connection from a system that is not recognized as authenticated by a known authority.

Prev | Up | Next
I.4.4.2 WS Interface | Home | I.5 Media Interchange

DICOM PS3.2 2016c - Conformance