DICOM PS3.2 2016c - Conformance

F.4.4.2 Parameters
Prev | F.4.4 Configuration | Next

#### F.4.4.2 Parameters

Table F.4.4-2. Configuration Parameters

Parameter | Configurable | Default Value
--- | --- | ---
General Parameters
Maximum PDU size I can receive | Yes | 128kbytes
Maximum PDU size I can send | Yes | 128kbytes
Time-out waiting for response to TCP/IP connect() request. (Low-level timeout) | Yes | 10 s
Time-out waiting for A-ASSOCIATE RQ PDU on open TCP/IP connection. (ARTIM timeout) | Yes | 30 s
Time-out waiting for acceptance or rejection response to an Association Open Request. (Application Level timeout) | Yes | 30s
Time-out waiting for acceptance of a TCP/IP message over the network. (Low-level timeout) | Yes | 30 s
Time-out for waiting for data between TCP/IP packets. (Low-level timeout) | Yes | 30 s
The Windows NT TCP/IP socket buffer size is set to 1,342,177 bytes in order to improve image data throughput performance. | No | 1,342,177 bytes
STORAGE-SCU AE Parameters
Maximum number of simultaneous Associations. | Yes | 10
STORAGE-SCU AE time-out waiting for a Response to a C-STORE-RQ. (DIMSE timeout) | Yes | 5 minutes
STORAGE-SCU AE number of times a failed send job to a C-MOVE Destination is automatically retried. | No | 0
STORAGE-SCP AE Parameters
Maximum PDU Size | Yes | 16384
Maximum number of simultaneous Associations (Can be configured to be a maximum total number or a maximum per external SCU AE) | Yes | 10
STORAGE-SCP AE time-out waiting on an open Association for the next Request message (C-STORE-RQ, Association Close Request. etc.) (DIMSE timeout) | Yes | 15 minutes
STORAGE-SCP AE maximum number of simultaneous Associations | Yes ### Note Can be configured with a maximum per external AE | 10
Permanent archival of SOP Instances sent by a peer AE to the STORAGE-SCP AE in response to a retrieval request from QUERY-RETRIEVE AE. | Yes | FALSE (Such received SOP Instances are not archived.)
Permanent archival of SOP Instances sent unsolicited by a peer AE to the STORAGE-SCP AE. I.e. Not in response to a retrieval request from QUERY-RETRIEVE AE. | Yes | TRUE (Such received SOP Instances are archived.)
Always open a new Association to send a Storage Commitment Push Model Notification request (N-EVENT-REPORT-RQ). | Yes | FALSE (Default is to try and send Notifications over original Association opened by peer AE).
Maximum number of times to attempt sending a Storage Commitment Push Model N-EVENT-REPORT Request when an error status is returned or communication failure occurs. | Yes | 5
Time to wait between attempts to send a Storage Commitment Push Model N-EVENT-REPORT Request when an error status is returned or communication failure occurs. | Yes | 5 minutes
QUERY-RETRIEVE-SCP AE Parameters
Maximum PDU Size | Yes | 16384
Maximum number of simultaneous Associations (Can be configured to be a maximum total number or a maximum per external SCU AE) | Yes | 10
QUERY-RETRIEVE-SCP AE time-out waiting on an open Association for the next message (C-FIND-RQ, C-MOVE-RQ, Association Close Request. etc.) (DIMSE timeout) | Yes | 3 minutes
QUERY-RETRIEVE-SCP AE maximum number of simultaneous Associations | Yes ### Note Can be configured with a maximum per external AE | 10

Prev | Up | Next
F.4.4 Configuration | Home | F.5 Media Interchange

DICOM PS3.2 2016c - Conformance