DICOM PS3.3 2016c - Information Object Definitions

C.17 SR Document Modules
Prev | C Information Module Definitions (Normative) | Next

## C.17 SR Document Modules

### C.17.1 SR Document Series Module

Table C.17-1 defines the Attributes of the SR Document Series. A Series of SR Documents may contain any number of SR Documents.

### Note

Series of SR Documents are separate from Series of Images or other Composite SOP Instances. SR Documents do not reside in a Series of Images or other Composite SOP Instances.

Table C.17-1. SR Document Series Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Modality | (0008,0060) | 1 | Modality type. Enumerated Values: SR SR Document
Series Instance UID | (0020,000E) | 1 | Unique identifier of the Series. ### Note No SR-specific semantics are specified.
Series Number | (0020,0011) | 1 | A number that identifies the Series. ### Note No SR-specific semantics are specified.
Series Date | (0008,0021) | 3 | Date the Series started.
Series Time | (0008,0031) | 3 | Time the Series started.
Protocol Name | (0018,1030) | 3 | Description of the conditions under which the Series was performed. ### Note This may represent the type of analysis used in creation of the SR SOP Instances.
Series Description | (0008,103E) | 3 | Description of the Series
Series Description Code Sequence | (0008,103F) | 3 | A coded description of the Series. Only a single Item is permitted in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” | No Baseline CID is defined.
Referenced Performed Procedure Step Sequence | (0008,1111) | 2 | Uniquely identifies the Performed Procedure Step SOP Instance for which the Series is created. Zero or one Item shall be included in this Sequence. ### Note The Performed Procedure Step referred to by this Attribute is the Step during which this Document is generated. If this Document is generated during the same Performed Procedure Step as the evidence in the current interpretation procedure, this attribute may contain reference to that Performed Procedure Step. This Attribute is not used to convey reference to the evidence in the current interpretation procedure. See Current Requested Procedure Evidence Sequence (0040,A375). This Sequence may be sent zero length if the Performed Procedure Step is unknown.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |

Prev | Up | Next
C.16 Stored Print Specific Modules | Home | C.17.2 SR Document General Module

DICOM PS3.3 2016c - Information Object Definitions