DICOM PS3.17 2016c - Explanatory Information

T.4.2 Interpolated Reference
Prev | T.4 Quantitative Arterial Analysis Reference Method | Next

### T.4.2 Interpolated Reference

The interpolated reference obstruction analysis calculates a reconstruction diameter for each position in the analyzed artery. This reconstructed diameter represents the diameters of the artery when no disease would be present. The reconstruction diameter is a line fitted through at least two user-defined reference markers by linear interpolation.

By default two references are used at the positions of the reference markers are automatically positioned at 5% and 95% of the artery length.

To calculate a percentage diameter stenosis the reference diameter for the obstruction is defined as the reconstructed diameter at the position of the MLD.

In cases where the proximal and distal part of the analyzed artery have a stable diameter during the treatment and long-term follow-up, this method will produce a stable reference diameter for all positions in the artery.

Prev | Up | Next
T.4 Quantitative Arterial Analysis Reference Method | Home | T.4.3 Mean Local Reference

DICOM PS3.17 2016c - Explanatory Information