DICOM PS3.10 2016c - Media Storage and File Format for Media Interchange

6.2.2 Media Format Layer
Prev | 6.2 The DICOM Media Storage Model | Next

### 6.2.2 Media Format Layer

At the Media Format Layer, Physical Media bit streams are organized into specific structures. Data file structures and associated directory structures are defined to allow efficient access and management of the physical media space.

### Note

This layer is often specific to a given operating system environment. An example of such a Media Format Layer definition associated with the 3 1/2 inch floppy disk are the data structures used by the operating systems of various personal computer file systems. PS3.12 and its annexes specify several Media Format choices.

Media Formats supported by the DICOM Standard are selected to support the minimum requirements specified by the DICOM File Service as specified in Section 8 of this Part. Constraining access to the File content through such a DICOM File Service ensures that the DICOM Data Format Layer is independent from Media Format and Physical Media selection.

Prev | Up | Next
6.2 The DICOM Media Storage Model | Home | 6.2.3 DICOM Data Format Layer

DICOM PS3.10 2016c - Media Storage and File Format for Media Interchange