DICOM PS3.16 2016c - Content Mapping Resource

CID 6135 Image Quality Finding
Prev | B DCMR Context Groups (Normative) | Next

## CID 6135 Image Quality Finding

Type:

  Extensible

Version:

  20090402

Table CID 6135. Image Quality Finding

Coding Scheme Designator | Code Value | Code Meaning
--- | --- | ---
DCM | 111208 | Grid artifact(s)
DCM | 111209 | Positioning
DCM | 111210 | Motion blur
DCM | 111211 | Under exposed
DCM | 111212 | Over exposed
DCM | 111213 | No image
DCM | 111214 | Detector artifact(s)
DCM | 111215 | Artifact(s) other than grid or detector artifact
DCM | 111216 | Mechanical failure
DCM | 111217 | Electrical failure
DCM | 111218 | Software failure
DCM | 111219 | Inappropriate image processing
DCM | 111220 | Other failure
DCM | 111221 | Unknown failure
RADLEX | RID11327 | Beam-hardening artifact

Prev | Up | Next
CID 6134 Chest Qualitative Temporal Difference Type | Home | CID 6136 Chest Types of Quality Control Standard

DICOM PS3.16 2016c - Content Mapping Resource