DICOM PS3.3 2016c - Information Object Definitions

C.8.25.16.6 Ophthalmic Axial Measurements Quality Image SOP Instance Reference Macro
Prev | C.8.25.16 Intraocular Lens Calculations Module | Next

##### C.8.25.16.6 Ophthalmic Axial Measurements Quality Image SOP Instance Reference Macro

Table C.8.25.16-6 describes the attributes for the Ophthalmic Axial Measurements Quality Image SOP Instance Reference Macro

Table C.8.25.16-6. Ophthalmic Axial Measurements Quality Image SOP Instance Reference Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Referenced SOP Class UID | (0008,1150) | 1 | Uniquely identifies the referenced SOP Class. Enumerated Values: 1.2.840.10008.5.1.4.1.1.7.2 Multi-frame Grayscale Byte Secondary Capture Image Storage 1.2.840.10008.5.1.4.1.1.7.4 Multi-frame True Color Secondary Capture Image Storage
Referenced SOP Instance UID | (0008,1155) | 1 | Uniquely identifies the referenced SOP Instance.
Referenced Frame Number | (0008,1160) | 1 | Identifies the frame number within the Referenced SOP Instance to which the reference applies. The first frame shall be denoted as frame number 1. Only a single value shall exist. ### Note This Attribute is a multi-value field but for this Macro it can only contain one value.

Prev | Up | Next
C.8.25.16.5 Calculated IOL Macro | Home | C.8.26 Visual Field Static Perimetry Measurements Modules

DICOM PS3.3 2016c - Information Object Definitions