DICOM PS3.3 2016c - Information Object Definitions

A.34.9.4.4 Sampling Frequency
Prev | A.34.9.4 Respiratory Waveform IOD Content Constraints | Next

##### A.34.9.4.4 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence Item shall be less than or equal to100 Hz.

Prev | Up | Next
A.34.9.4.3 Number of Waveform Channels | Home | A.34.9.4.5 Channel Source

DICOM PS3.3 2016c - Information Object Definitions