DICOM PS3.11 2016c - Media Storage Application Profiles

B.3.2 Physical Media and Media Formats
Prev | B.3 STD-XA1K Application Profile Class Requirements | Next

### B.3.2 Physical Media and Media Formats

The 1024 X-Ray Angiographic Application CD-R Profile STD-XA1K-CD requires the 120mm CD-R physical media with the ISO/IEC 9660 Media Format, as defined in PS3.12.

The 1024 X-Ray Angiographic Application DVD profile STD-XA1K-DVD requires any of the 120 mm DVD media other than DVD-RAM as defined in PS3.12.

Prev | Up | Next
B.3 STD-XA1K Application Profile Class Requirements | Home | B.3.3 Directory Information in DICOMDIR

DICOM PS3.11 2016c - Media Storage Application Profiles