DICOM PS3.16 2016c - Content Mapping Resource

CID 9403 IEC61217 Patient Support Position Parameters
Prev | B DCMR Context Groups (Normative) | Next

## CID 9403 IEC61217 Patient Support Position Parameters

Type:

  Extensible

Version:

  20130518

Table CID 9403. IEC61217 Patient Support Position Parameters

Coding Scheme Designator | Code Value | Code Meaning
--- | --- | ---
DCM | 126801 | IEC61217 Patient Support Continuous Angle
DCM | 126802 | IEC61217 Table Top Continuous Pitch Angle
DCM | 126803 | IEC61217 Table Top Continuous Roll Angle
DCM | 126804 | IEC61217 Table Top Eccentric Axis Distance
DCM | 126805 | IEC61217 Table Top Continuous Eccentric Angle
DCM | 126806 | IEC61217 Table Top Lateral Position
DCM | 126807 | IEC61217 Table Top Longitudinal Position
DCM | 126808 | IEC61217 Table Top Vertical Position

Prev | Up | Next
CID 9402 IEC61217 Gantry Position Parameters | Home | CID 10000 Scope of Accumulation

DICOM PS3.16 2016c - Content Mapping Resource