DICOM PS3.15 2016c - Security and System Management Profiles

B.7 Generic SAML Assertion Identity Negotiation Association Profile
Prev | B Secure Transport Connection Profiles (Normative) | Next

## B.7 Generic SAML Assertion Identity Negotiation Association Profile

An implementation that supports the Generic SAML Assertion Identity Negotiation Association Profile shall send/accept the User Identity association negotiation sub-item, for User-Identity-Type of 4. If a positive response is requested, the association acceptor implementation shall respond with the association response sub-item containing a SAML response. The SAML Assertion information shall be made available to internal or external authentication systems. The user identity shall be authenticated by means of an authentication system that employs SAML Assertions. If the authentication fails, the association shall be rejected.

The user identity from the Primary-field shall be used within the implementation as the user identification. Such uses include recording user identification in audit messages.

Table B.7-1. Generic SAML Assertion Identity Negotiation Association Profile - Minimum Mechanisms for DICOM Association Negotiation Features

Supported Association Negotiation Feature | Minimum Mechanism
--- | ---
User Identity | SAML Assertion

Prev | Up | Next
B.6 Kerberos Identity Negotiation Association Profile | Home | B.8 Secure Use of Email Transport

DICOM PS3.15 2016c - Security and System Management Profiles