DICOM PS3.3 2016c - Information Object Definitions

C.11.11 Presentation State Relationship Module
Prev | C.11 Look Up Tables and Presentation States | Next

### C.11.11 Presentation State Relationship Module

Table C.11.11-1 contains Attributes that describe the images to which a Presentation State applies.

Table C.11.11-1. Presentation State Relationship Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Include Table C.11.11-1b “Presentation State Relationship Macro Attributes” |

Table C.11.11-1b. Presentation State Relationship Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Referenced Series Sequence | (0008,1115) | 1 | Sequence of Items where each Item includes the Attributes of one Series to which the Presentation applies. One or more Items shall be included in this Sequence.
>Series Instance UID | (0020,000E) | 1 | Unique identifier of a Series that is part of the Study defined by the Study Instance UID (0020,000D) in the enclosing data set. ### Note The Study Instance UID (0020,000D) value will be that of the presentation state itself, unless the macro is invoked from Blending Sequence (0070,0402) in the Presentation State Blending Module, in which case it will be explicitly specified.
>Referenced Image Sequence | (0008,1140) | 1 | The set of images and frames to which the Presentation applies. These shall be of the Study defined by Study Instance UID (0020,000D) and the Series defined by Series Instance UID (0020,000E). One or more Items shall be included in this Sequence. The referenced SOP Class shall be the same for all Images in any Item of this Referenced Series Sequence (0008,1115).
>>Include Table 10-3 “Image SOP Instance Reference Macro Attributes” |

Prev | Up | Next
C.11.10 Presentation State Identification Module | Home | C.11.12 Presentation State Shutter Module

DICOM PS3.3 2016c - Information Object Definitions