DICOM PS3.3 2016d - Information Object Definitions

C.8.8.19 Measured Dose Reference Record Module
Prev | C.8.8 Radiotherapy Modules | Next

#### C.8.8.19 Measured Dose Reference Record Module

Table C.8-55. Measured Dose Reference Record Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Measured Dose Reference Sequence | (3008,0010) | 1 | Sequence of doses measured during treatment delivery, summed over entire session. One or more Items shall be included in this Sequence.
>Referenced Dose Reference Number | (300C,0051) | 1C | Uniquely identifies Dose Reference specified by Dose Reference Number (300A,0012) in Dose Reference Sequence (300A,0010) in RT Prescription Module of referenced RT Plan. Required only if Measured Dose Reference Number (3008,0064) is not sent. It shall not be present otherwise.
>Measured Dose Reference Number | (3008,0064) | 1C | Unique identifier of measured dose point. Required only if Referenced Dose Reference Number (300C,0051) is not sent. It shall not be present otherwise.
>Dose Units | (3004,0002) | 1 | Units used to describe measured dose. Enumerated Values: GY Gray RELATIVE Dose relative to implicit reference value
>Measured Dose Value | (3008,0016) | 2 | Measured Dose in units specified by Dose Units (3004,0002).
>Measured Dose Type | (3008,0014) | 2 | Type of dose measurement. Defined Terms: DIODE semiconductor diode TLD thermoluminescent dosimeter ION_CHAMBER ion chamber GEL dose sensitive gel EPID electronic portal imaging device FILM dose sensitive film
>Measured Dose Description | (3008,0012) | 3 | User-defined description of Dose Reference (e.g., "Exit dose", "Point A").

Prev | Up | Next
C.8.8.18 RT Treatment Machine Record Module | Home | C.8.8.20 Calculated Dose Reference Record Module

DICOM PS3.3 2016d - Information Object Definitions