DICOM PS3.16 2016d - Content Mapping Resource

TID 3313 Stress ECG Summary
Prev | Stress Testing Report Templates | Next

### TID 3313 Stress ECG Summary

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3313. Stress ECG Summary

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | TEXT | EV (F-00033, SRT, "ECG Finding") | 1 | U |  | Device Generated Test Summary
2 | > | HAS OBS CONTEXT | CODE | EV (121005, DCM, "Observer Type") | 1 | M |  | EV (121007, DCM, "Device")
3 | > | HAS OBS CONTEXT | INCLUDE | DTID 1004 “Device Observer Identifying Attributes” | 1 | M |  |
4 |  |  | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = EV (F-03204, SRT, "ST Elevation") $Units = DT (mV, UCUM, "mV") $Derivation = EV (G-A437, SRT, "Maximum") $TargetSite = DCID 3001 “ECG Leads”
5 |  |  | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = EV (F-38279, SRT, "ST Depression") $Units = DT (mV, UCUM, "mV") $Derivation = EV (G-A437, SRT, "Maximum") $TargetSite = DCID 3001 “ECG Leads”
6 |  |  | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = EV (F-38287, SRT, "T wave alternans") $Units = DT (uV, UCUM, "uV") $Derivation = EV (G-A437, SRT, "Maximum") $TargetSite = DCID 3001 “ECG Leads”
7 |  |  | CODE | EV (F-38035, SRT, "ST Segment Finding") | 1 | U |  | BCID 3231 “ST Segment Findings”
8 | > | HAS PROPERTIES | CODE | EV (G-C0E3, SRT, "Finding Site") | 1-n | U |  | BCID 3232 “ST Segment Location”
9 | > | HAS PROPERTIES | CODE | EV (G-C504, SRT, "Associated Morphology") | 1 | U |  | BCID 3233 “ST Segment Morphology”
10 |  |  | NUM | DT (122707, DCM, "Number of Ectopic Beats") | 1 | U |  | UNITS = EV ({beats}, UCUM, "beats")
11 | > | HAS PROPERTIES | CODE | EV (G-C504, SRT, "Associated Morphology") | 1-n | U |  | BCID 3234 “Ectopic Beat Morphology”
12 |  |  | CODE | DT (8884-9, LN, "Cardiac Rhythm") | 1-2 | U |  | BCID 3415 “Cardiac Rhythms” See note.
13 | > | HAS CONCEPT MOD | CODE | EV (109054, DCM, "Patient State") | 1 | M |  | DCID 3102 “Rest-Stress”
14 |  |  | CODE | EV (F-00033, SRT, "ECG Finding") | 1-n | U |  | BCID 3230 “ECG Findings”
15 | > | HAS CONCEPT MOD | CODE | EV (109054, DCM, "Patient State") | 1 | U |  | BCID 3262 “ECG Patient State Values”

Content Item Descriptions

Rows 4-14 | Each observation (measurement or finding) may have a specific Content Item Observation DateTime attribute to indicate the time in the procedure at which the observation was made (e.g., time of maximum heart rate, or time of occurrence of an arrhythmia).
Row 12-13 | This Concept and the associated Concept Modifier may be instantiated twice, once for resting state measurements, once for stress.

Prev | Up | Next
TID 3312 Physiological Summary | Home | TID 3317 Stress Imaging Summary

DICOM PS3.16 2016d - Content Mapping Resource